March 25, 2015

* Want to store data in the same way throughout sampling period; this will make offloading data much easier
* Think about just running device until battery dies and looking at time stamps for power testing.
* Try adjusting microcontroller frequency to save power
* Programming hard reset: could be internal issue to microcontroller
* Get part orders to Schafer
* Make sure via holes are large enough for 22-gauge wire