(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.600198)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Front")
		(1 "In1.Cu" power)
		(2 "In2.Cu" power)
		(31 "B.Cu" signal "Back")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 0.480066)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "prepreg")
				(thickness 0.480066)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "core")
				(thickness 0.480066)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "charmv7parts/")
		)
	)
	(net 0 "")
	(net 1 "/1.8V")
	(net 2 "/SCL")
	(net 3 "/SDA")
	(net 4 "/LED_DEBUG")
	(net 5 "unconnected-(U9-IO45-Pad26)")
	(net 6 "GND")
	(net 7 "/REGOUT_1")
	(net 8 "unconnected-(U9-IO10-Pad18)")
	(net 9 "unconnected-(U9-IO9-Pad17)")
	(net 10 "unconnected-(U9-IO11-Pad19)")
	(net 11 "unconnected-(U9-IO36-Pad29)")
	(net 12 "/VUSB")
	(net 13 "Net-(J25-Pin_1)")
	(net 14 "/NSL_UART_RX")
	(net 15 "unconnected-(U9-IO35-Pad28)")
	(net 16 "/NSL_UART_RTS")
	(net 17 "/NSL_UART_CTS")
	(net 18 "Net-(LED1-A)")
	(net 19 "/NSL_UART_TX")
	(net 20 "Net-(J26-Pin_2)")
	(net 21 "unconnected-(J1-Pin_15-Pad15)")
	(net 22 "unconnected-(J10-SBU2-PadB8)")
	(net 23 "/3V3")
	(net 24 "/NSL_5V")
	(net 25 "/5V")
	(net 26 "unconnected-(J1-Pin_1-Pad1)")
	(net 27 "unconnected-(J10-TX1+-PadA2)")
	(net 28 "/NSL_3V3")
	(net 29 "Net-(J14-Pin_2)")
	(net 30 "unconnected-(J1-Pin_2-Pad2)")
	(net 31 "unconnected-(J10-RX2+-PadA11)")
	(net 32 "unconnected-(J10-RX1+-PadB11)")
	(net 33 "/D_N")
	(net 34 "/D_P")
	(net 35 "Net-(J10-CC1)")
	(net 36 "unconnected-(J10-TX2--PadB3)")
	(net 37 "unconnected-(J10-TX2+-PadB2)")
	(net 38 "Net-(J10-CC2)")
	(net 39 "unconnected-(J10-RX2--PadA10)")
	(net 40 "unconnected-(J10-TX1--PadA3)")
	(net 41 "unconnected-(J10-RX1--PadB10)")
	(net 42 "unconnected-(J10-SBU1-PadA8)")
	(net 43 "Net-(SJ1-A)")
	(net 44 "Net-(SJ2-A)")
	(net 45 "unconnected-(U5-NC-Pad2)")
	(net 46 "/BOOT")
	(net 47 "/RESET")
	(net 48 "unconnected-(J1-Pin_17-Pad17)")
	(net 49 "unconnected-(J1-Pin_18-Pad18)")
	(net 50 "/REGOUT_2")
	(net 51 "/INT1_2")
	(net 52 "/IMU_WAKEUP_2")
	(net 53 "/MAG_WAKEUP")
	(net 54 "unconnected-(U1-NC-Pad2)")
	(net 55 "Net-(U5-C1)")
	(net 56 "Net-(LED2-A)")
	(net 57 "/INT1_1")
	(net 58 "unconnected-(U1-RESV-Pad19)")
	(net 59 "unconnected-(U1-NC-Pad5)")
	(net 60 "unconnected-(U1-NC-Pad3)")
	(net 61 "unconnected-(U1-NC-Pad17)")
	(net 62 "unconnected-(U1-NC-Pad16)")
	(net 63 "unconnected-(U1-NC-Pad14)")
	(net 64 "unconnected-(U1-AUX_DA-Pad21)")
	(net 65 "unconnected-(U1-NC-Pad4)")
	(net 66 "unconnected-(U1-AUX_CL-Pad7)")
	(net 67 "unconnected-(U1-NC-Pad1)")
	(net 68 "unconnected-(U1-NC-Pad6)")
	(net 69 "unconnected-(U1-NC-Pad15)")
	(net 70 "unconnected-(U5-NC-Pad11)")
	(net 71 "unconnected-(U5-NC-Pad12)")
	(net 72 "unconnected-(U9-IO3-Pad15)")
	(net 73 "unconnected-(U9-IO46-Pad16)")
	(net 74 "Net-(LED4-A)")
	(net 75 "/A3")
	(net 76 "/A0")
	(net 77 "/A2")
	(net 78 "/A1")
	(net 79 "Net-(J14-Pin_1)")
	(net 80 "Net-(J15-Pin_2)")
	(net 81 "Net-(J15-Pin_1)")
	(net 82 "Net-(J16-Pin_1)")
	(net 83 "Net-(J16-Pin_2)")
	(net 84 "unconnected-(U11-BO1-Pad11)")
	(net 85 "unconnected-(U11-BO2-Pad7)")
	(net 86 "/DIR2_Z")
	(net 87 "/DIR1_Z")
	(net 88 "/PWM_Z")
	(net 89 "/STBY_ZA")
	(net 90 "/DIR1_X")
	(net 91 "/PWM_X")
	(net 92 "/DIR2_X")
	(net 93 "/STBY_XY")
	(net 94 "/PWM_Y")
	(net 95 "/DIR2_Y")
	(net 96 "/DIR1_Y")
	(net 97 "Net-(LED5-A)")
	(net 98 "Net-(R28-Pad1)")
	(net 99 "Net-(R29-Pad1)")
	(net 100 "Net-(R30-Pad1)")
	(net 101 "unconnected-(U11-BIN2-Pad16)")
	(net 102 "unconnected-(U10-NC-Pad5)")
	(net 103 "unconnected-(U10-NC-Pad16)")
	(net 104 "unconnected-(U10-AUX_CL-Pad7)")
	(net 105 "unconnected-(U10-RESV-Pad19)")
	(net 106 "unconnected-(U10-AUX_DA-Pad21)")
	(net 107 "unconnected-(U10-NC-Pad15)")
	(net 108 "unconnected-(U10-NC-Pad4)")
	(net 109 "unconnected-(U10-NC-Pad2)")
	(net 110 "unconnected-(U10-NC-Pad6)")
	(net 111 "unconnected-(U10-NC-Pad3)")
	(net 112 "unconnected-(U10-NC-Pad14)")
	(net 113 "unconnected-(U10-NC-Pad1)")
	(net 114 "unconnected-(U10-NC-Pad17)")
	(net 115 "/IMU_WAKEUP_1")
	(net 116 "/SDA_1V8_1")
	(net 117 "/SDA_1V8_2")
	(net 118 "/SCL_1V8_1")
	(net 119 "/SCL_1V8_2")
	(net 120 "/AD0_1")
	(net 121 "/AD0_2")
	(net 122 "unconnected-(U11-BIN1-Pad17)")
	(net 123 "unconnected-(U11-BO2-Pad7)_1")
	(net 124 "unconnected-(U11-BO1-Pad11)_1")
	(net 125 "unconnected-(U11-PWMB-Pad15)")
	(net 126 "Net-(J3-Pin_1)")
	(net 127 "Net-(J27-Pin_2)")
	(net 128 "Net-(JP1-A)")
	(net 129 "Net-(JP2-A)")
	(net 130 "Net-(LEDUSB1-A)")
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 85.6 53.65 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -0.05 -0.95 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/RESET")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 88 104.1555)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -0.0125 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "Net-(SJ1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 89.9 57.6 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LEDUSB1"
			(at -1.55 0.975 180)
			(layer "F.SilkS")
		)
		(property "Value" "Yellow USB Connection Indicator"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB" "C375438"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "Net-(LEDUSB1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 116.562 57.05 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.574 -0.338 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "/INT1_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 118.15 82.55 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 2.4 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "imagery:charmslogo"
		(layer "F.Cu")
		(at 114.2 123.95)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "StockLib:JST04_1MM_RA"
		(layer "F.Cu")
		(at 89 120.55 180)
		(property "Reference" "J11"
			(at -2.35 -4.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "JST_SH_4"
			(at 0 3.46555 0)
			(layer "F.Fab")
		)
		(property "Footprint" "StockLib:JST04_1MM_RA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -2.8 1.6)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S2" smd rect
			(at 2.8 1.6)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "SHIELD__1")
			(pintype "passive")
		)
		(model "../StockLib.3dshapes/SM04B-SRSS-TB_LF__SN_.step"
			(offset
				(xyz 0 1.5 -0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 87.04 46.424 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 80.55 102.95 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 1.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/BOOT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 115.2 83.4 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 2.45 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "StockLib:Jumper_NO_Small"
		(layer "F.Cu")
		(at 90.6 104.1555)
		(property "Reference" "SJ1"
			(at 1.75 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNP"
			(at 0.31 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "StockLib:Jumper_NO_Small"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 43 "Net-(SJ1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 109.774 49.528501 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at -1.552501 1 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "/SCL_1V8_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 98.9 70.05 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at -2.9 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "Net-(R29-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(J15-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 114.974 54.376)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0.3 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 104.725 96.7 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J27"
			(at 0 5.225 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "Net-(J27-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 112.7 85.85 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "/STBY_ZA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "StockLib:JST04_1MM_RA"
		(layer "F.Cu")
		(at 97.8 120.525 180)
		(property "Reference" "J4"
			(at -2.6 -4.275 0)
			(layer "F.SilkS")
		)
		(property "Value" "JST_SH_4"
			(at 0 3.46555 0)
			(layer "F.Fab")
		)
		(property "Footprint" "StockLib:JST04_1MM_RA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -2.8 1.6)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S2" smd rect
			(at 2.8 1.6)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "SHIELD__1")
			(pintype "passive")
		)
		(model "../StockLib.3dshapes/SM04B-SRSS-TB_LF__SN_.step"
			(offset
				(xyz 0 1.5 -0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 72.55 41.6 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 3.45 0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU Level Shifters:DIO_RB558WMF_ROM"
		(layer "F.Cu")
		(at 86.880001 41.262)
		(tags "RE1C002UNTCL ")
		(property "Reference" "R25"
			(at -1.728002 -0.938 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RE1C002UNTCL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU Level Shifters:DIO_RB558WMF_ROM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "RE1C002UNTCL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIO_RB558WMF_ROM DIO_RB558WMF_ROM-M DIO_RB558WMF_ROM-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.499999 0.762)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "GATE")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.499999 0.762)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "/SDA_1V8_2")
			(pinfunction "SOURCE")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 -0.762)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "DRAIN")
			(pintype "unspecified")
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 107.552499 52.309751)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -0.102499 1.264249 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/SDA_1V8_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 98.8 106.875 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0.05 1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" ".1 uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 114.3 108.075 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 3.675 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 13 "Net-(J25-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 107.1 70.05)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 2.85 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "Net-(R28-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(J14-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 80.6 109.05)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 1.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/BOOT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 110.8 98.025 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J25"
			(at 0.1 -2.625 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J25-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 82.3 45.075 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 3.075 -0.15 180)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 116.25 83.4 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 2.4 -0.15 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.33 91.85 90)
		(descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x04 2.54mm single row")
		(property "Reference" "J12"
			(at 0.475 -2.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Socket"
			(at 0 10.39 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 113.8 65.9)
		(descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH side entry")
		(property "Reference" "J16"
			(at 5.45 0.2 -90)
			(layer "F.SilkS")
		)
		(property "Value" "MTQ_Z"
			(at 1 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 82 "Net-(J16-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "Net-(J16-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 77.4 43.375 90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U8"
			(at 3.275 4.7 180)
			(layer "F.SilkS")
		)
		(property "Value" "AMS1117-1.8"
			(at 0 4.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Low Dropout regulator, positive, 1.8V fixed output, SOT-223"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at 3.15 0 90)
			(size 2 3.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_GCT_USB4115-03-C"
		(layer "F.Cu")
		(at 85.45 63.79)
		(descr "USB TYPE C, VERT RCPT PCB, SMT, https://gct.co/files/drawings/usb4115.pdf")
		(tags "USB C Type-C Receptacle SMD")
		(property "Reference" "J10"
			(at 5.65 -1.305 90)
			(layer "F.SilkS")
		)
		(property "Value" "USB_C_Receptacle"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_USB:USB_C_Receptacle_GCT_USB4115-03-C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB Full-Featured Type-C Receptacle connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -3.75 0)
			(size 0.66 0.66)
			(drill 0.66)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 3.75 0)
			(size 1 0.58)
			(drill oval 1 0.58)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -2.75 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A2" smd rect
			(at -2.25 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "unconnected-(J10-TX1+-PadA2)")
			(pinfunction "TX1+")
			(pintype "bidirectional+no_connect")
		)
		(pad "A3" smd rect
			(at -1.75 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "unconnected-(J10-TX1--PadA3)")
			(pinfunction "TX1-")
			(pintype "bidirectional+no_connect")
		)
		(pad "A4" smd rect
			(at -1.25 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/VUSB")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd rect
			(at -0.75 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(J10-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "/D_P")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at 0.25 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/D_N")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd rect
			(at 0.75 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "unconnected-(J10-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A9" smd rect
			(at 1.25 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/VUSB")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A10" smd rect
			(at 1.75 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "unconnected-(J10-RX2--PadA10)")
			(pinfunction "RX2-")
			(pintype "bidirectional+no_connect")
		)
		(pad "A11" smd rect
			(at 2.25 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "unconnected-(J10-RX2+-PadA11)")
			(pinfunction "RX2+")
			(pintype "bidirectional+no_connect")
		)
		(pad "A12" smd rect
			(at 2.75 -0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd rect
			(at 2.75 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B2" smd rect
			(at 2.25 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "unconnected-(J10-TX2+-PadB2)")
			(pinfunction "TX2+")
			(pintype "bidirectional+no_connect")
		)
		(pad "B3" smd rect
			(at 1.75 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "unconnected-(J10-TX2--PadB3)")
			(pinfunction "TX2-")
			(pintype "bidirectional+no_connect")
		)
		(pad "B4" smd rect
			(at 1.25 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/VUSB")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd rect
			(at 0.75 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(J10-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.25 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "/D_P")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at -0.25 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/D_N")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at -0.75 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "unconnected-(J10-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B9" smd rect
			(at -1.25 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/VUSB")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B10" smd rect
			(at -1.75 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "unconnected-(J10-RX1--PadB10)")
			(pinfunction "RX1-")
			(pintype "bidirectional+no_connect")
		)
		(pad "B11" smd rect
			(at -2.25 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "unconnected-(J10-RX1+-PadB11)")
			(pinfunction "RX1+")
			(pintype "bidirectional+no_connect")
		)
		(pad "B12" smd rect
			(at -2.75 0.835)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole circle
			(at -2.4 -2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole circle
			(at -2.4 2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole circle
			(at 2.4 -2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole circle
			(at 2.4 2.15)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(name "peg")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 86.25 61.99) (xy 84.65 61.99) (xy 84.65 61.29) (xy 86.25 61.29)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(name "peg")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 86.25 66.29) (xy 84.65 66.29) (xy 84.65 65.59) (xy 86.25 65.59)
				)
			)
		)
		(model "G:/Shared drives/IrishSat/13.0 NearSpace/Design/EESD/CHARMSat_AidanV4/Parts/LIB_USB4115-03-C/USB4115-03-C/3D/USB4115-03-C.stp"
			(offset
				(xyz -28.5 -17.5 -0.91)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 103.95 83.28 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 2.42 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 76.2 81.35 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.9 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 107.05 82.57 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 77.7 68.225 180)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J24"
			(at -0.008986 -2.618986 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/D_P")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/D_N")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/VUSB")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 89.066 40.924 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at -1.599999 0.776 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "/SCL_1V8_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 111.897101 58.7029 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.7 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/REGOUT_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.69 48.174 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -1.95 -0.088001 -90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/INT1_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 91.09 48.274 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 2.35 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/REGOUT_2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU Level Shifters:DIO_RB558WMF_ROM"
		(layer "F.Cu")
		(at 111.774 49.550001 -90)
		(tags "RE1C002UNTCL ")
		(property "Reference" "R24"
			(at 0.849999 -1.876 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RE1C002UNTCL"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU Level Shifters:DIO_RB558WMF_ROM"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "RE1C002UNTCL"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIO_RB558WMF_ROM DIO_RB558WMF_ROM-M DIO_RB558WMF_ROM-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.499999 0.762 270)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "GATE")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.499999 0.762 270)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 118 "/SCL_1V8_1")
			(pinfunction "SOURCE")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 -0.762 270)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "DRAIN")
			(pintype "unspecified")
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 96.2 65.95)
		(descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH side entry")
		(property "Reference" "J15"
			(at 5.4 0.75 -90)
			(layer "F.SilkS")
		)
		(property "Value" "MTQ_Y"
			(at 1 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 81 "Net-(J15-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "Net-(J15-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1210_3225Metric"
		(layer "F.Cu")
		(at 98.55 112.3)
		(descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0.125 2.425 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_1210_3225Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 128 "Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 127 "Net-(J27-Pin_2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 82.2 68.025 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/VUSB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 102.21 91.95 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at 0.05 -2.66 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 109.4 106.75 90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U2"
			(at 3.65 4.675 180)
			(layer "F.SilkS")
		)
		(property "Value" "AMS1117-3.3"
			(at 0 4.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J26-Pin_2)")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at 3.15 0 90)
			(size 2 3.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J26-Pin_2)")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J25-Pin_1)")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU Level Shifters:DIO_RB558WMF_ROM"
		(layer "F.Cu")
		(at 93.74 48.174 90)
		(tags "RE1C002UNTCL ")
		(property "Reference" "R4"
			(at 1.55 1.561999 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RE1C002UNTCL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU Level Shifters:DIO_RB558WMF_ROM"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "RE1C002UNTCL"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIO_RB558WMF_ROM DIO_RB558WMF_ROM-M DIO_RB558WMF_ROM-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.499999 0.762 90)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "GATE")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.499999 0.762 90)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "/INT1_2")
			(pinfunction "SOURCE")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 -0.762 90)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/IMU_WAKEUP_2")
			(pinfunction "DRAIN")
			(pintype "unspecified")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 94.35 113.6 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0 2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 128 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 28 "/NSL_3V3")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 127 "Net-(J27-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 70.65 40.6175 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 1.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(LED4-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU Level Shifters:DIO_RB558WMF_ROM"
		(layer "F.Cu")
		(at 90.978 40.874 -90)
		(tags "RE1C002UNTCL ")
		(property "Reference" "R27"
			(at 0 -2.05 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RE1C002UNTCL"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU Level Shifters:DIO_RB558WMF_ROM"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "RE1C002UNTCL"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIO_RB558WMF_ROM DIO_RB558WMF_ROM-M DIO_RB558WMF_ROM-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.499999 0.762 270)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "GATE")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.499999 0.762 270)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 119 "/SCL_1V8_2")
			(pinfunction "SOURCE")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 -0.762 270)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "DRAIN")
			(pintype "unspecified")
		)
	)
	(footprint "ESP32-S3:XCVR_ESP32-S3-WROOM-1-N16R2"
		(layer "F.Cu")
		(at 86.65 85.95)
		(property "Reference" "U9"
			(at 8.675 14.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "ESP32-S3-WROOM-1-N16R2"
			(at 7.395 14.365 0)
			(layer "F.Fab")
		)
		(property "Footprint" "ESP32-S3:XCVR_ESP32-S3-WROOM-1-N16R2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Espressif Systems"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.25mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "NON STANDARD Espressif Systems"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ESP32-S3-WROOM-1-N16R2/Espressif+Systems/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "v1.0"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ESP32-S3-WROOM-1-N16R2/Espressif+Systems/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "ESP32-S3-WROOM-1-N16R2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "\n                        \n                            Bluetooth, WiFi 802.11b/g/n, Bluetooth v5.0 Transceiver Module 2.4GHz PCB Trace Surface Mount\n                        \n"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Espressif"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "ANTENNA"
			(at -4.5 -9.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -8.75 -5.26)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -8.75 -3.99)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "3V3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -8.75 -2.72)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/RESET")
			(pinfunction "EN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -8.75 -1.45)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/NSL_UART_CTS")
			(pinfunction "IO4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -8.75 -0.18)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/NSL_UART_RTS")
			(pinfunction "IO5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -8.75 1.09)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/NSL_UART_RX")
			(pinfunction "IO6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -8.75 2.36)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/NSL_UART_TX")
			(pinfunction "IO7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -8.75 3.63)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/LED_DEBUG")
			(pinfunction "IO15")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -8.75 4.9)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "/A1")
			(pinfunction "IO16")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at -8.75 6.17)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "/A0")
			(pinfunction "IO17")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at -8.75 7.44)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "/A3")
			(pinfunction "IO18")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at -8.75 8.71)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "/A2")
			(pinfunction "IO8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at -8.75 9.98)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/D_N")
			(pinfunction "IO19")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at -8.75 11.25)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "/D_P")
			(pinfunction "IO20")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at -6.985 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "unconnected-(U9-IO3-Pad15)")
			(pinfunction "IO3")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at -5.715 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "unconnected-(U9-IO46-Pad16)")
			(pinfunction "IO46")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at -4.445 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U9-IO9-Pad17)")
			(pinfunction "IO9")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at -3.175 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U9-IO10-Pad18)")
			(pinfunction "IO10")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd rect
			(at -1.905 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "unconnected-(U9-IO11-Pad19)")
			(pinfunction "IO11")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd rect
			(at -0.635 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "/STBY_ZA")
			(pinfunction "IO12")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd rect
			(at 0.635 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "/PWM_Z")
			(pinfunction "IO13")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd rect
			(at 1.905 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "/DIR2_Z")
			(pinfunction "IO14")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd rect
			(at 3.175 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "/DIR1_Z")
			(pinfunction "IO21")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd rect
			(at 4.445 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "IO47")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "25" smd rect
			(at 5.715 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "IO48")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "26" smd rect
			(at 6.985 12.5)
			(size 0.9 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "unconnected-(U9-IO45-Pad26)")
			(pinfunction "IO45")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "27" smd rect
			(at 8.75 11.25)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/BOOT")
			(pinfunction "IO0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "28" smd rect
			(at 8.75 9.98)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "unconnected-(U9-IO35-Pad28)")
			(pinfunction "IO35")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "29" smd rect
			(at 8.75 8.71)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U9-IO36-Pad29)")
			(pinfunction "IO36")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "30" smd rect
			(at 8.75 7.44)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "/DIR1_X")
			(pinfunction "IO37")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "31" smd rect
			(at 8.75 6.17)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "/DIR2_X")
			(pinfunction "IO38")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "32" smd rect
			(at 8.75 4.9)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "/PWM_X")
			(pinfunction "IO39")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "33" smd rect
			(at 8.75 3.63)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "/STBY_XY")
			(pinfunction "IO40")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "34" smd rect
			(at 8.75 2.36)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "/DIR1_Y")
			(pinfunction "IO41")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "35" smd rect
			(at 8.75 1.09)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "/DIR2_Y")
			(pinfunction "IO42")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "36" smd rect
			(at 8.75 -0.18)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "/PWM_Y")
			(pinfunction "RXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "37" smd rect
			(at 8.75 -1.45)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "/IMU_WAKEUP_1")
			(pinfunction "TXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "38" smd rect
			(at 8.75 -2.72)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/MAG_WAKEUP")
			(pinfunction "IO2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "39" smd rect
			(at 8.75 -3.99)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/IMU_WAKEUP_2")
			(pinfunction "IO1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "40" smd rect
			(at 8.75 -5.26)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_1" smd rect
			(at -1.5 2.46)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_2" smd rect
			(at -2.9 2.46)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_3" smd rect
			(at -0.1 2.46)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_4" smd rect
			(at -2.9 3.86)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_5" smd rect
			(at -1.5 3.86)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_6" smd rect
			(at -0.1 3.86)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_7" smd rect
			(at -2.9 1.06)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_8" smd rect
			(at -1.5 1.06)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_9" smd rect
			(at -0.1 1.06)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "41_10" thru_hole circle
			(at -1.5 1.76)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_11" thru_hole circle
			(at -2.9 1.76)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_12" thru_hole circle
			(at -0.1 1.76)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_13" thru_hole circle
			(at -2.9 3.16)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_14" thru_hole circle
			(at -1.5 3.16)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_15" thru_hole circle
			(at -0.1 3.16)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_16" thru_hole circle
			(at -2.2 1.06)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_17" thru_hole circle
			(at -0.8 1.06)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_18" thru_hole circle
			(at -2.2 2.46)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_19" thru_hole circle
			(at -0.8 2.46)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_20" thru_hole circle
			(at -2.2 3.86)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(pad "41_21" thru_hole circle
			(at -0.8 3.86)
			(size 0.4 0.4)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 77.65 73.2) (xy 95.65 73.2) (xy 95.65 79.2) (xy 77.65 79.2)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 77.65 73.2) (xy 95.65 73.2) (xy 95.65 79.2) (xy 77.65 79.2)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 77.65 73.2) (xy 95.65 73.2) (xy 95.65 79.2) (xy 77.65 79.2)
				)
			)
		)
		(model "G:/Shared drives/IrishSat/13.0 NearSpace/Design/EESD/CHARMSat_AidanV8_ESP32/Parts/ESP32-S3-WROOM-1-N16R2/ESP32-S3-WROOM-1-N16R2.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 88.05 57.525 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0.6 1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "Net-(LEDUSB1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/VUSB")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 99.65 83.95 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 3.05 0.15 180)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 25 "/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_LGA:LGA-12_2x2mm_P0.5mm"
		(layer "F.Cu")
		(at 102.4 40.942899 -90)
		(descr "LGA12")
		(tags "lga land grid array")
		(property "Reference" "U5"
			(at -0.098298 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "LIS2MDL"
			(at 0 1.6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_LGA:LGA-12_2x2mm_P0.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lis2mdl.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra-low-power, 3-axis digital output magnetometer, LGA-12"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LGA*2x2mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7625 -0.75 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "SCL/SPC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.7625 -0.25 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "unconnected-(U5-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd rect
			(at -0.7625 0.25 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -0.7625 0.75 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "SDA/SDI/SDO")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -0.25 0.7625)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(U5-C1)")
			(pinfunction "C1")
			(pintype "power_out")
		)
		(pad "6" smd rect
			(at 0.25 0.7625)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at 0.7625 0.75 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/MAG_WAKEUP")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 0.7625 0.25 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.7625 -0.25 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "Vdd")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at 0.7625 -0.75 270)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "Vdd_IO")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at 0.25 -0.7625)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "unconnected-(U5-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" smd rect
			(at -0.25 -0.7625)
			(size 0.375 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "unconnected-(U5-NC-Pad12)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1210_3225Metric"
		(layer "F.Cu")
		(at 95.35 108.025)
		(descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at -0.075 2.325 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_1210_3225Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 129 "Net-(JP2-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 126 "Net-(J3-Pin_1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 104.55 105.05 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 3.325 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 20 "Net-(J26-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 58.08 124.44 90)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "J6"
			(at 1.27 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x04_Odd_Even"
			(at 1.27 9.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/NSL_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/NSL_3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/NSL_UART_RTS")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/NSL_UART_CTS")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/NSL_UART_TX")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/NSL_UART_RX")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 103.25 43.342899 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0.301702 -1.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 99.92 40.692899 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0.45 -1.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "Net-(U5-C1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "StockLib:Jumper_NO_Small"
		(layer "F.Cu")
		(at 92.7375 104.1555 180)
		(property "Reference" "SJ2"
			(at 1.6 0 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DNP"
			(at 0.31 3.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "StockLib:Jumper_NO_Small"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 44 "Net-(SJ2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "StockLib:Jumper_NO_Small"
		(layer "F.Cu")
		(at 110.724 56.800001 -90)
		(property "Reference" "SJ3"
			(at 0.752899 1.676899 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DNP"
			(at 0.31 3.4 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "StockLib:Jumper_NO_Small"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 120 "/AD0_1")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 6 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 101.6 85.9 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 2.85 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "/STBY_XY")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 116.55 70.05 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at -2.85 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "Net-(R30-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "Net-(J16-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 88 69.575)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 2.9175 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "Net-(J10-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104.95 83.3 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 2.4 -0.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 99.605 110.075)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at -0.025 -1.025 0)
			(layer "F.SilkS")
		)
		(property "Value" ".1 uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "Net-(J27-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 94.4 102.375 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -0.625 -1.425 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "Net-(SJ2-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 70.65 42.585 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED4"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Red"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(LED4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "StockLib:Jumper_NO_Small"
		(layer "F.Cu")
		(at 89.49 48.274 -90)
		(property "Reference" "SJ4"
			(at 1.65 0.238001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DNP"
			(at 0.31 3.4 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "StockLib:Jumper_NO_Small"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 121 "/AD0_2")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "StockLib:JST04_1MM_RA"
		(layer "F.Cu")
		(at 80.05 120.55 180)
		(property "Reference" "J2"
			(at -2.85 -4.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "JST_SH_4"
			(at 0 3.46555 0)
			(layer "F.Fab")
		)
		(property "Footprint" "StockLib:JST04_1MM_RA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.5 -2.275 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/SCL")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -2.8 1.6)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S2" smd rect
			(at 2.8 1.6)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "SHIELD__1")
			(pintype "passive")
		)
		(model "../StockLib.3dshapes/SM04B-SRSS-TB_LF__SN_.step"
			(offset
				(xyz 0 1.5 -0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 93.65 45.124 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0.7 1.151999 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 50.2 93.4775 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -2.04 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/LED_DEBUG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "Net-(LED2-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 88.75 68.025)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.6 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/VUSB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 50.25 101.32125 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at -2.57125 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "Net-(LED5-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 50.2 115.635 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at -2.665 -1.7 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Green"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU:QFN24_3X3X0P9_IVS"
		(layer "F.Cu")
		(at 111.7 53.5)
		(tags "ICM-20948 ")
		(property "Reference" "U1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ICM-20948"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU:QFN24_3X3X0P9_IVS"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ICM-20948"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN24_3X3X0P9_IVS QFN24_3X3X0P9_IVS-M QFN24_3X3X0P9_IVS-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.4892 -1.2 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.1938 -1.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.1938 -1.2 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.524 -1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "unconnected-(U1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -1.524 -0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "unconnected-(U1-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd rect
			(at -1.524 -0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "unconnected-(U1-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "4" smd rect
			(at -1.524 0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "unconnected-(U1-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd rect
			(at -1.524 0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "unconnected-(U1-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd rect
			(at -1.524 1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "unconnected-(U1-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd rect
			(at -1.000001 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "unconnected-(U1-AUX_CL-Pad7)")
			(pinfunction "AUX_CL")
			(pintype "unspecified+no_connect")
		)
		(pad "8" smd rect
			(at -0.599999 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "VDDIO")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at -0.2 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "/AD0_1")
			(pinfunction "SDO/AD0")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 0.2 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/REGOUT_1")
			(pinfunction "REGOUT")
			(pintype "output")
		)
		(pad "11" smd rect
			(at 0.599999 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "FSYNC")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 1.000001 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/INT1_1")
			(pinfunction "INT1")
			(pintype "output")
		)
		(pad "13" smd rect
			(at 1.524 1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 1.524 0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "unconnected-(U1-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" smd rect
			(at 1.524 0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "unconnected-(U1-NC-Pad15)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "16" smd rect
			(at 1.524 -0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "unconnected-(U1-NC-Pad16)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "17" smd rect
			(at 1.524 -0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "unconnected-(U1-NC-Pad17)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "18" smd rect
			(at 1.524 -1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "19" smd rect
			(at 1.000001 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "unconnected-(U1-RESV-Pad19)")
			(pinfunction "RESV")
			(pintype "no_connect")
		)
		(pad "20" smd rect
			(at 0.599999 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "RESV_GND")
			(pintype "power_out")
		)
		(pad "21" smd rect
			(at 0.2 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "unconnected-(U1-AUX_DA-Pad21)")
			(pinfunction "AUX_DA")
			(pintype "unspecified+no_connect")
		)
		(pad "22" smd rect
			(at -0.2 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "nCS")
			(pintype "input")
		)
		(pad "23" smd rect
			(at -0.599999 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 118 "/SCL_1V8_1")
			(pinfunction "SCL/SCLK")
			(pintype "input")
		)
		(pad "24" smd rect
			(at -1.000001 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "/SDA_1V8_1")
			(pinfunction "SDA/SDI")
			(pintype "input")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 110.8999 52.6999) (xy 112.5001 52.6999) (xy 112.5001 54.3001) (xy 110.8999 54.3001)
				)
			)
		)
		(model "G:/Shared drives/IrishSat/13.0 NearSpace/Design/EESD/CHARMSat_AidanV4/Parts/ICM-20948/ICM-20948--3DModel-STEP-269445.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 86.88 43.174)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at -1.578001 0.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "/SDA_1V8_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 83.7 60.025 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 2.4 0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(J10-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "StockLib:KMR_2"
		(layer "F.Cu")
		(at 80.9 106 180)
		(descr "KMR_2")
		(tags "Switch")
		(property "Reference" "SW2"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "KMR231GLFS"
			(at -0.28 -5.7 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "StockLib:KMR_2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "C&K KMR2 KMR4"
			(at 0.29 4.17 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.8 -2.05 90)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0.8 -2.05 90)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/BOOT")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0.8 2.05 90)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/BOOT")
			(pinfunction "3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -0.8 2.05 90)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "../StockLib.3dshapes/KMR441GLFS.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
		(layer "F.Cu")
		(at 114.1 76.8 -90)
		(descr "24-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SSOP 0.65")
		(property "Reference" "U11"
			(at 0 -5.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TB6612FNG"
			(at 0 5.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/us/product/linear/motordriver/detail.TB6612FNG.html"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Driver IC for Dual DC motor, SSOP-24"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP-24*5.3x8.2mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.6 -3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 100 "Net-(R30-Pad1)")
			(pinfunction "AO1")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -3.6 -2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 100 "Net-(R30-Pad1)")
			(pinfunction "AO1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.6 -2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND1")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -3.6 -1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -3.6 -0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "Net-(J16-Pin_1)")
			(pinfunction "AO2")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -3.6 -0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "Net-(J16-Pin_1)")
			(pinfunction "AO2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -3.6 0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "unconnected-(U11-BO2-Pad7)_1")
			(pinfunction "BO2")
			(pintype "output+no_connect")
		)
		(pad "8" smd rect
			(at -3.6 0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "unconnected-(U11-BO2-Pad7)")
			(pinfunction "BO2")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at -3.6 1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND2")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at -3.6 2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND2")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -3.6 2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "unconnected-(U11-BO1-Pad11)")
			(pinfunction "BO1")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at -3.6 3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "unconnected-(U11-BO1-Pad11)_1")
			(pinfunction "BO1")
			(pintype "passive+no_connect")
		)
		(pad "13" smd rect
			(at 3.6 3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/5V")
			(pinfunction "VM2")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 3.6 2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/5V")
			(pinfunction "VM3")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 3.6 2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 125 "unconnected-(U11-PWMB-Pad15)")
			(pinfunction "PWMB")
			(pintype "input+no_connect")
		)
		(pad "16" smd rect
			(at 3.6 1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "unconnected-(U11-BIN2-Pad16)")
			(pinfunction "BIN2")
			(pintype "input+no_connect")
		)
		(pad "17" smd rect
			(at 3.6 0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 122 "unconnected-(U11-BIN1-Pad17)")
			(pinfunction "BIN1")
			(pintype "input+no_connect")
		)
		(pad "18" smd rect
			(at 3.6 0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at 3.6 -0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "/STBY_ZA")
			(pinfunction "STBY")
			(pintype "input")
		)
		(pad "20" smd rect
			(at 3.6 -0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "21" smd rect
			(at 3.6 -1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "/DIR1_Z")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "22" smd rect
			(at 3.6 -2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "/DIR2_Z")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "23" smd rect
			(at 3.6 -2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "/PWM_Z")
			(pinfunction "PWMA")
			(pintype "input")
		)
		(pad "24" smd rect
			(at 3.6 -3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/5V")
			(pinfunction "VM1")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU Level Shifters:DIO_RB558WMF_ROM"
		(layer "F.Cu")
		(at 114.612 57.05 90)
		(tags "RE1C002UNTCL ")
		(property "Reference" "R8"
			(at 0.2971 -1.914899 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RE1C002UNTCL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU Level Shifters:DIO_RB558WMF_ROM"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "RE1C002UNTCL"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIO_RB558WMF_ROM DIO_RB558WMF_ROM-M DIO_RB558WMF_ROM-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.499999 0.762 90)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "GATE")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.499999 0.762 90)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/INT1_1")
			(pinfunction "SOURCE")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 -0.762 90)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "/IMU_WAKEUP_1")
			(pinfunction "DRAIN")
			(pintype "unspecified")
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 50.25 103.25375 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED5"
			(at -0.7675 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Green"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "Net-(LED5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 110.75 83.95 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 3 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 25 "/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 113.274 58.600001 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.05 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "/IMU_WAKEUP_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 116.75 95.5)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J26"
			(at 0 5.15 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J26-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 50.2 113.66 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 4.44 -0.15 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/NSL_5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(LED1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 92.39 50.174 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -0.05 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/IMU_WAKEUP_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 90.25 108.7 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at -0.05 -1.95 90)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0 2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 129 "Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 24 "/NSL_5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 126 "Net-(J3-Pin_1)")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 101 43.392899 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0.901702 1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "/MAG_WAKEUP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "StockLib:KMR_2"
		(layer "F.Cu")
		(at 82.4 54 90)
		(descr "KMR_2")
		(tags "Switch")
		(property "Reference" "SW1"
			(at 2.45 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "KMR231GLFS"
			(at -0.28 -5.7 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "StockLib:KMR_2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "C&K KMR2 KMR4"
			(at 0.29 4.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.8 -2.05)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0.8 -2.05)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/RESET")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0.8 2.05)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/RESET")
			(pinfunction "3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -0.8 2.05)
			(size 0.9 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "../StockLib.3dshapes/KMR441GLFS.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 56.57 46.8 90)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "J5"
			(at 1.27 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x04_Odd_Even"
			(at 1.27 9.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/PWM_Z")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/PWM_X")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "/PWM_Y")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SCL")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
		(layer "F.Cu")
		(at 103 76.8 -90)
		(descr "24-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SSOP 0.65")
		(property "Reference" "U6"
			(at 0 -5.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TB6612FNG"
			(at 0 5.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/us/product/linear/motordriver/detail.TB6612FNG.html"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Driver IC for Dual DC motor, SSOP-24"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP-24*5.3x8.2mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.6 -3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "Net-(R28-Pad1)")
			(pinfunction "AO1")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -3.6 -2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "Net-(R28-Pad1)")
			(pinfunction "AO1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.6 -2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND1")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -3.6 -1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -3.6 -0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "Net-(J14-Pin_1)")
			(pinfunction "AO2")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -3.6 -0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "Net-(J14-Pin_1)")
			(pinfunction "AO2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -3.6 0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "Net-(J15-Pin_1)")
			(pinfunction "BO2")
			(pintype "output")
		)
		(pad "8" smd rect
			(at -3.6 0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "Net-(J15-Pin_1)")
			(pinfunction "BO2")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -3.6 1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND2")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at -3.6 2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "PGND2")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -3.6 2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "Net-(R29-Pad1)")
			(pinfunction "BO1")
			(pintype "output")
		)
		(pad "12" smd rect
			(at -3.6 3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "Net-(R29-Pad1)")
			(pinfunction "BO1")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 3.6 3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/5V")
			(pinfunction "VM2")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 3.6 2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/5V")
			(pinfunction "VM3")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 3.6 2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "/PWM_Y")
			(pinfunction "PWMB")
			(pintype "input")
		)
		(pad "16" smd rect
			(at 3.6 1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "/DIR2_Y")
			(pinfunction "BIN2")
			(pintype "input")
		)
		(pad "17" smd rect
			(at 3.6 0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "/DIR1_Y")
			(pinfunction "BIN1")
			(pintype "input")
		)
		(pad "18" smd rect
			(at 3.6 0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at 3.6 -0.325 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "/STBY_XY")
			(pinfunction "STBY")
			(pintype "input")
		)
		(pad "20" smd rect
			(at 3.6 -0.975 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "21" smd rect
			(at 3.6 -1.625 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "/DIR1_X")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "22" smd rect
			(at 3.6 -2.275 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "/DIR2_X")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "23" smd rect
			(at 3.6 -2.925 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "/PWM_X")
			(pinfunction "PWMA")
			(pintype "input")
		)
		(pad "24" smd rect
			(at 3.6 -3.575 270)
			(size 1.75 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/5V")
			(pinfunction "VM1")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU:QFN24_3X3X0P9_IVS"
		(layer "F.Cu")
		(at 90.85 44.7)
		(tags "ICM-20948 ")
		(property "Reference" "U10"
			(at 4.201999 -2.676 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ICM-20948"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU:QFN24_3X3X0P9_IVS"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ICM-20948"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN24_3X3X0P9_IVS QFN24_3X3X0P9_IVS-M QFN24_3X3X0P9_IVS-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.4892 -1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.1938 -1.2 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.1938 -1.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.524 -1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "unconnected-(U10-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -1.524 -0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "unconnected-(U10-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd rect
			(at -1.524 -0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "unconnected-(U10-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "4" smd rect
			(at -1.524 0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "unconnected-(U10-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd rect
			(at -1.524 0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "unconnected-(U10-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd rect
			(at -1.524 1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "unconnected-(U10-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd rect
			(at -1.000001 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 104 "unconnected-(U10-AUX_CL-Pad7)")
			(pinfunction "AUX_CL")
			(pintype "unspecified+no_connect")
		)
		(pad "8" smd rect
			(at -0.599999 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "VDDIO")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at -0.2 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "/AD0_2")
			(pinfunction "SDO/AD0")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 0.2 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/REGOUT_2")
			(pinfunction "REGOUT")
			(pintype "output")
		)
		(pad "11" smd rect
			(at 0.599999 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "FSYNC")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 1.000001 1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "/INT1_2")
			(pinfunction "INT1")
			(pintype "output")
		)
		(pad "13" smd rect
			(at 1.524 1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 1.524 0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "unconnected-(U10-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" smd rect
			(at 1.524 0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "unconnected-(U10-NC-Pad15)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "16" smd rect
			(at 1.524 -0.2 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "unconnected-(U10-NC-Pad16)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "17" smd rect
			(at 1.524 -0.599999 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "unconnected-(U10-NC-Pad17)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "18" smd rect
			(at 1.524 -1.000001 90)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "19" smd rect
			(at 1.000001 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "unconnected-(U10-RESV-Pad19)")
			(pinfunction "RESV")
			(pintype "no_connect")
		)
		(pad "20" smd rect
			(at 0.599999 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "GND")
			(pinfunction "RESV_GND")
			(pintype "power_out")
		)
		(pad "21" smd rect
			(at 0.2 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 106 "unconnected-(U10-AUX_DA-Pad21)")
			(pinfunction "AUX_DA")
			(pintype "unspecified+no_connect")
		)
		(pad "22" smd rect
			(at -0.2 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "nCS")
			(pintype "input")
		)
		(pad "23" smd rect
			(at -0.599999 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 119 "/SCL_1V8_2")
			(pinfunction "SCL/SCLK")
			(pintype "input")
		)
		(pad "24" smd rect
			(at -1.000001 -1.524)
			(size 0.2032 0.6604)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "/SDA_1V8_2")
			(pinfunction "SDA/SDI")
			(pintype "input")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 90.0499 43.8999) (xy 91.6501 43.8999) (xy 91.6501 45.5001) (xy 90.0499 45.5001)
				)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 105.05 65.95)
		(descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH side entry")
		(property "Reference" "J14"
			(at 5.25 0.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "MTQ_X"
			(at 1 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 79 "Net-(J14-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J14-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 79.2 53.7 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.17 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/RESET")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.3 44.538678 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 2.35 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 50.2 95.4275 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED2"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Blue"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "Net-(LED2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 107.847101 55.2029 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "IMU Level Shifters:DIO_RB558WMF_ROM"
		(layer "F.Cu")
		(at 107.573999 50.359751)
		(tags "RE1C002UNTCL ")
		(property "Reference" "R21"
			(at -1.823999 -0.985751 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RE1C002UNTCL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "IMU Level Shifters:DIO_RB558WMF_ROM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "RE1C002UNTCL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIO_RB558WMF_ROM DIO_RB558WMF_ROM-M DIO_RB558WMF_ROM-L")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.499999 0.762)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/1.8V")
			(pinfunction "GATE")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.499999 0.762)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "/SDA_1V8_1")
			(pinfunction "SOURCE")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 -0.762)
			(size 0.3556 0.5842)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SDA")
			(pinfunction "DRAIN")
			(pintype "unspecified")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 73.346898 110.001619 90)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "J1"
			(at 1.27 2.87 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 -25.19 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "CHARM_ESP32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -11.43 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(J1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/A2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/A3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/A0")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/A1")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/NSL_UART_TX")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/NSL_UART_RX")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/NSL_UART_RTS")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/NSL_UART_CTS")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 -15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 -15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 -17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J1-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole oval
			(at 2.54 -17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 -20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(J1-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
		)
		(pad "18" thru_hole oval
			(at 2.54 -20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(J1-Pin_18-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
		)
		(pad "19" thru_hole oval
			(at 0 -22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/NSL_3V3")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 2.54 -22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/NSL_5V")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "imagery:lgcharmslogo"
		(layer "B.Cu")
		(at 83.357934 78.049145 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_arc
		(start 35.890698 129.7369)
		(mid 34.473802 129.149996)
		(end 33.886898 127.7331)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 122.386898 126.7369)
		(end 121.031898 126.7369)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 33.886898 36.2407)
		(mid 34.473807 34.823809)
		(end 35.890698 34.2369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 47.486898 126.3769)
		(end 45.936898 126.3769)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.386898 120.001619)
		(end 130.886898 114.501619)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 33.886898 36.2407)
		(end 33.886898 127.7331)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 40.886898 131.7407)
		(end 40.886898 132.9869)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.886898 49.472181)
		(end 125.386898 43.972181)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.386898 36.240698)
		(end 125.386898 43.972181)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 40.886898 30.9869)
		(end 40.886898 32.2331)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 47.486898 37.5969)
		(end 45.936898 37.5969)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 120.566798 114.546)
		(end 119.016798 114.546)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 38.883098 34.2369)
		(end 35.890698 34.2369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.890698 129.7369)
		(end 38.883098 129.7369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.383098 34.2369)
		(mid 124.800002 34.823795)
		(end 125.386898 36.240698)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.383098 34.2369)
		(end 115.651617 34.2369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 36.886898 126.7369)
		(end 35.531898 126.7369)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 40.886898 132.9869)
		(end 112.401617 132.9869)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 125.386898 127.7331)
		(mid 124.800009 129.150009)
		(end 123.3831 129.7369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 40.886898 32.2331)
		(mid 40.300008 33.65001)
		(end 38.883098 34.2369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.3831 129.7369)
		(end 115.651617 129.7369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.386898 127.7331)
		(end 125.386898 120.001619)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.401617 30.9869)
		(end 40.886898 30.9869)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.651617 34.2369)
		(end 112.401617 30.9869)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 122.386898 37.2369)
		(end 121.031898 37.2369)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 120.566798 49.4278)
		(end 119.016798 49.4278)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 36.886898 37.2369)
		(end 35.531898 37.2369)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 38.883098 129.7369)
		(mid 40.300002 130.323796)
		(end 40.886898 131.7407)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.401617 132.9869)
		(end 115.651617 129.7369)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.886898 114.501619)
		(end 130.886898 49.472181)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_text "CHARMS"
		(at 82 40 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 67 106.05 0)
		(layer "B.SilkS")
	)
	(gr_text "Aidan Oblepias, Isaac Brej, Peter Gibbons, Sarah Kopfer\nJackson O'Neill, John Tuma, Robby Diamond, Tyler Hanson\nAndrew Gaylord, David Scully, Patrick Schwartz, Peyton Reynolds"
		(at 82 120 0)
		(layer "B.SilkS")
	)
	(gr_text "RTS"
		(at 61.8 112.5 0)
		(layer "B.SilkS")
	)
	(gr_text "A1"
		(at 69 106.05 0)
		(layer "B.SilkS")
	)
	(gr_text "TX"
		(at 64 112.5 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 67.05 112.45 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 59.5 112.55 0)
		(layer "B.SilkS")
	)
	(gr_text "A2"
		(at 71.6 112.45 0)
		(layer "B.SilkS")
	)
	(gr_text "A0"
		(at 69.1 112.45 0)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 51.6 112.6 0)
		(layer "B.SilkS")
	)
	(gr_text "ThinSat Payload MotherBoard\nUniversity of Notre Dame\n\n"
		(at 82 55.4 0)
		(layer "B.SilkS")
	)
	(gr_text "CTS"
		(at 61.916898 106.131619 0)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 51.15 105.95 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 58.15 105.85 0)
		(layer "B.SilkS")
	)
	(gr_text "RX"
		(at 64.1 106.05 0)
		(layer "B.SilkS")
	)
	(gr_text "A3"
		(at 71.55 106.05 0)
		(layer "B.SilkS")
	)
	(gr_text "A0"
		(at 67.45 112.1 0)
		(layer "F.SilkS")
	)
	(gr_text "NSL 3V3"
		(at 87.7 114.15 0)
		(layer "F.SilkS")
	)
	(gr_text "CTS"
		(at 59.25 106.4 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 109.95 89.75 0)
		(layer "F.SilkS")
	)
	(gr_text "DN"
		(at 75.2 96.45 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 55.15 49.85 0)
		(layer "F.SilkS")
	)
	(gr_text "IMU 1"
		(at 104.8 60.95 0)
		(layer "F.SilkS")
	)
	(gr_text "VUSB"
		(at 71.5 60.95 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.25 106.15 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA P.U."
		(at 86.1375 106.2055 0)
		(layer "F.SilkS")
	)
	(gr_text "Y"
		(at 58.55 42.1 0)
		(layer "F.SilkS")
	)
	(gr_text "Z"
		(at 56 42.05 0)
		(layer "F.SilkS")
	)
	(gr_text "L"
		(at 87.6 107.9 0)
		(layer "F.SilkS")
	)
	(gr_text "X"
		(at 58.55 49.9 0)
		(layer "F.SilkS")
	)
	(gr_text "ESP32-S3-WROOM-1\n"
		(at 78.4 72.85 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 64.7 118.5 0)
		(layer "F.SilkS")
	)
	(gr_text "D1Y"
		(at 96.3 88.9 0)
		(layer "F.SilkS")
	)
	(gr_text "NSL BUS PINS"
		(at 57.1 104.4 0)
		(layer "F.SilkS")
	)
	(gr_text "A1"
		(at 67.55 106.25 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3 LDO"
		(at 106.6 112.6 0)
		(layer "F.SilkS")
	)
	(gr_text "P_X"
		(at 96.35 91.4 0)
		(layer "F.SilkS")
	)
	(gr_text "NSL3V3"
		(at 49 112.7 0)
		(layer "F.SilkS")
	)
	(gr_text "RTS"
		(at 59.25 112.35 0)
		(layer "F.SilkS")
	)
	(gr_text "NSL ACCESS PINS"
		(at 56.15 116.5 0)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 64.75 119.8 0)
		(layer "F.SilkS")
	)
	(gr_text "AUX"
		(at 96.7 117.25 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 58.75 119.85 0)
		(layer "F.SilkS")
	)
	(gr_text "Z"
		(at 113.5 63.89 0)
		(layer "F.SilkS")
	)
	(gr_text "A3"
		(at 75.3 93.95 0)
		(layer "F.SilkS")
	)
	(gr_text "NSL5V"
		(at 54.1 119.9 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 63.25 49.9 0)
		(layer "F.SilkS")
	)
	(gr_text "5VPWR"
		(at 49.45 116.7375 90)
		(layer "F.SilkS")
	)
	(gr_text "D1X"
		(at 96.35 93.95 0)
		(layer "F.SilkS")
	)
	(gr_text "A0"
		(at 75.3 92.65 0)
		(layer "F.SilkS")
	)
	(gr_text "D2X"
		(at 96.35 92.7 0)
		(layer "F.SilkS")
	)
	(gr_text "RTS"
		(at 61.75 119.8 0)
		(layer "F.SilkS")
	)
	(gr_text "20"
		(at 75.35 107.95 0)
		(layer "F.SilkS")
	)
	(gr_text "BYPASS"
		(at 84.2 110.55 0)
		(layer "F.SilkS")
	)
	(gr_text "Y"
		(at 104.75 63.94 0)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 92.85 101.95 90)
		(layer "F.SilkS")
	)
	(gr_text "DP"
		(at 75.2 97.6 0)
		(layer "F.SilkS")
	)
	(gr_text "D1Z"
		(at 90.35 102.05 90)
		(layer "F.SilkS")
	)
	(gr_text "A2"
		(at 70 112.1 0)
		(layer "F.SilkS")
	)
	(gr_text "BOOT"
		(at 83.8 107.9 90)
		(layer "F.SilkS")
	)
	(gr_text "NSL 5V"
		(at 84.35 109.25 0)
		(layer "F.SilkS")
	)
	(gr_text "A3"
		(at 70.05 106.3 0)
		(layer "F.SilkS")
	)
	(gr_text "D2Z"
		(at 89.05 102.05 90)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 117.85 89.75 0)
		(layer "F.SilkS")
	)
	(gr_text "CHARMS"
		(at 78.3 36.65 0)
		(layer "F.SilkS")
	)
	(gr_text "5VDISC.\n"
		(at 101.3 94.8 0)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 60.25 42.1 0)
		(layer "F.SilkS")
	)
	(gr_text "CAMERA 2"
		(at 86 117.25 0)
		(layer "F.SilkS")
	)
	(gr_text "IMU 2"
		(at 89.55 53.9 0)
		(layer "F.SilkS")
	)
	(gr_text "X"
		(at 95.9 63.94 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 47.95 108.1 0)
		(layer "F.SilkS")
	)
	(gr_text "RESET"
		(at 80.1 57.15 0)
		(layer "F.SilkS")
	)
	(gr_text "CHARM V2.1 CDH PCB"
		(at 102.716587 125.45 45)
		(layer "F.SilkS")
	)
	(gr_text "SCL P.U."
		(at 91.7375 106.2055 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 60.1 49.9 0)
		(layer "F.SilkS")
	)
	(gr_text "D1Y"
		(at 96.3 87.65 0)
		(layer "F.SilkS")
	)
	(gr_text "BYPASS"
		(at 88.25 115.45 0)
		(layer "F.SilkS")
	)
	(gr_text "CAMERA 1"
		(at 76.95 117.25 0)
		(layer "F.SilkS")
	)
	(gr_text "P_Z"
		(at 87.75 102 90)
		(layer "F.SilkS")
	)
	(gr_text "USB 2.0"
		(at 85.2 60.25 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 91.6 102 90)
		(layer "F.SilkS")
	)
	(gr_text "STZ_"
		(at 86.55 102.5 90)
		(layer "F.SilkS")
	)
	(gr_text "1V8 LDO"
		(at 78 49.2 0)
		(layer "F.SilkS")
	)
	(gr_text "MAG."
		(at 103.6 46.5 0)
		(layer "F.SilkS")
	)
	(gr_text "LDO OUT\n"
		(at 119.6 99.35 90)
		(layer "F.SilkS")
	)
	(gr_text "NSL3V3"
		(at 53.25 118.5 0)
		(layer "F.SilkS")
	)
	(gr_text "0.5MM CLR."
		(at 51.45 53.5 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 75.25 110.6 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 62.2 112.3 0)
		(layer "F.SilkS")
	)
	(gr_text "STXY"
		(at 96.35 90.15 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3DISC."
		(at 100.85 99.6 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 112.7 89.75 0)
		(layer "F.SilkS")
	)
	(gr_text "A2\n"
		(at 75.3 95.2 0)
		(layer "F.SilkS")
	)
	(gr_text "L"
		(at 91.6 112.8 0)
		(layer "F.SilkS")
	)
	(gr_text "BLINK15"
		(at 49.45 96.9 90)
		(layer "F.SilkS")
	)
	(gr_text "MTQ DEBUG"
		(at 56.6 40 0)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 115.3 89.7 0)
		(layer "F.SilkS")
	)
	(gr_text "NSL5V"
		(at 49.45 106.1 0)
		(layer "F.SilkS")
	)
	(gr_text "USB_DN"
		(at 69.9 66.35 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 58.8 118.4 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 63.3 42.1 0)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 62.4 106.45 0)
		(layer "F.SilkS")
	)
	(gr_text "CTS"
		(at 61.75 118.45 0)
		(layer "F.SilkS")
	)
	(gr_text "GND\n"
		(at 72.15 63.7 0)
		(layer "F.SilkS")
	)
	(gr_text "LDO IN"
		(at 113.85 98.8 90)
		(layer "F.SilkS")
	)
	(gr_text "3V3PWR"
		(at 49.55 104.7425 90)
		(layer "F.SilkS")
	)
	(gr_text "A1"
		(at 75.3 91.35 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 47.95 110.45 0)
		(layer "F.SilkS")
	)
	(gr_text "USB_DP"
		(at 69.95 68.85 0)
		(layer "F.SilkS")
	)
	(zone
		(net 6)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 16.002 6.802) (xy 16.002 210.952) (xy 19.302 214.252) (xy 215.852 214.252) (xy 292.302 137.802)
				(xy 292.302 36.002) (xy 263.102 6.802)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/3V3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 9.5 221.4) (xy 13.65 225.55) (xy 234.1 225.55) (xy 304.7 154.95) (xy 304.7 51.3) (xy 253.65 0.25)
				(xy 9.5 0.25)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 19.702 -3.586) (xy 19.702 206.614) (xy 24.202 211.114) (xy 274.265092 211.114) (xy 286.563959 199.311127)
				(xy 288.167697 7.664084) (xy 277.739414 -3.586)
			)
		)
	)
)
