(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(Q2-S)")
	(net 3 "+6V")
	(net 4 "VDD")
	(net 5 "+3.3V")
	(net 6 "+BATT")
	(net 7 "VBUS")
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "01a7ccc7-1418-4442-a542-b24afa7a1002")
		(at 159.3 62.775 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(uuid "ab816c72-fdef-4af1-99b2-26a855416abb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10u"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "11aa5471-8a7a-4aa6-80e2-f055867d9037")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f7a219d-c0d2-49d9-9e8f-710c1f75bf11")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "d0b123fd-4f69-43cd-9fd0-74fcf387149a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/dd0cc5c1-5fd2-411e-9ef9-cb9788562956")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c61109f7-526b-4fe7-825c-f89c76531e63")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9af1b00d-d018-4c58-82b9-f8665d3e5173")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4ee1e6ea-2adc-4d68-86fc-8a6c163975df")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a48ea4c8-0357-4e35-a9ce-1b1a2429a5e4")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffad8175-23bb-4dfb-b251-cf85552b84ab")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "69e7560a-700b-4cfd-918f-f988750d896f")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0133e94-b7b5-44fe-9b43-e2552cb7623a")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb86f330-9b13-46fd-a5a3-63138856fce8")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d32758dd-98bf-48fb-89d6-ed998af22205")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "023c5022-a506-48ec-8bf3-53401369cf7c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "22917225-ee8f-4c7e-a1a0-61e352e827fa")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 4 "VDD")
			(pintype "passive")
			(uuid "5655a378-93a9-4b6c-8299-e1c871c1f023")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(uuid "4b27364a-328d-4c28-a6cd-5563cc5b94ac")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "15d4a193-cc39-46b3-98b7-4b9ebf8773cc")
		(at 157.5 42)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "ca562383-1207-43a5-bd97-1618e31252d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" ".33u"
			(at 0 1.85 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e1d3bf5-3b02-4eb2-8873-4e7f415affd1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "495756df-a4a2-4e77-b416-45fad0a37d10")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dcc89d07-fd1b-483a-90f7-0d71d562789e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3c24211e-6f85-47e3-84af-83ad643942fd")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ab53ceb-f39d-44fe-89c7-6f9ec13cfb69")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6afdf7b7-8c37-4b14-a7f8-d8d42f9130eb")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "390a5cfb-c7e8-4f57-9c5a-59bb085ab152")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d010e3d-0168-463a-8b9b-cb36059b8689")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f1b57f51-3091-4334-bff7-b037fa08c459")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6d2ee9b-6146-4ed4-9bc1-ed871fc44b32")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14a34672-c0d7-4934-9e6f-07394c76dfd1")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71dfcd3c-eeec-4425-9254-e83aae97a006")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da4eb691-748e-46ca-b87d-664037c33773")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4dec6cd2-113f-4878-b99f-f94d32b599fb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "621b60d5-b46f-4df3-8ead-8b416a1a3c31")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "+6V")
			(pintype "passive")
			(uuid "0f2ac476-9a9e-46c7-812c-9f8a88e43d54")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(uuid "3852a5fa-6d0b-44d4-9d58-87036fde40b0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TO-263-2"
		(layer "F.Cu")
		(uuid "2171e029-8f47-4af5-9743-439f84915a42")
		(at 142.96 53.65 -90)
		(descr "TO-263/D2PAK/DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
		(tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
		(property "Reference" "U1"
			(at 0 -6.65 90)
			(layer "F.SilkS")
			(uuid "dacb845f-2f42-4284-9561-c0aa374eb472")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "L7806"
			(at 0 6.65 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "54beb46b-0abe-40d4-bd02-3ae483301ca8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d0004f5-c617-46a1-9f88-fde02e0ae37a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 6V, TO-220/TO-263/TO-252"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "65a40029-6112-4509-9add-4b22605262dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(path "/3d04e100-2b53-48ac-b549-aff56b6526ab")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.825 5.2)
			(end -4.825 3.39)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39ec1b63-6d28-4e7b-a62f-7fb8bd3f67a4")
		)
		(fp_line
			(start -3.46 5.2)
			(end -4.825 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6c235ce-b614-498e-b275-0b863e9bd70e")
		)
		(fp_line
			(start -4.825 -5.2)
			(end -4.825 -3.39)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "256ec554-91a5-495d-8d83-5f8016a68fbb")
		)
		(fp_line
			(start -3.46 -5.2)
			(end -4.825 -5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91f4abcb-04f9-4228-adc4-f2d6e257e9dc")
		)
		(fp_poly
			(pts
				(xy -7.65 -3.35) (xy -7.99 -3.82) (xy -7.31 -3.82)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "1f813c5d-1df1-4934-860f-0294e68a9ff9")
		)
		(fp_rect
			(start -10.2 -5.65)
			(end 6.45 5.65)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "b3b411e7-469e-40fe-a77f-0eb1274ea079")
		)
		(fp_line
			(start 5.625 5)
			(end 4.625 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ebc0977-b230-49be-9a8a-608a19b36987")
		)
		(fp_line
			(start -9.325 3.04)
			(end -4.625 3.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa64bac9-53fb-4a72-9d8b-8b44a4fc761a")
		)
		(fp_line
			(start -9.325 2.04)
			(end -9.325 3.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03c2545e-ef20-4c58-9083-0a6d0a9426b7")
		)
		(fp_line
			(start -4.625 2.04)
			(end -9.325 2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8af6741b-c1da-4c95-a8df-3899b0f04c77")
		)
		(fp_line
			(start -9.325 -2.04)
			(end -4.625 -2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47860641-e1fe-4cbf-ac54-d92b91cc6111")
		)
		(fp_line
			(start -9.325 -3.04)
			(end -9.325 -2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f601f25e-4a8d-4f1a-8241-c71d7de1947f")
		)
		(fp_line
			(start -4.625 -3.04)
			(end -9.325 -3.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "354455e9-34b2-45ee-8d70-b8ccbb7c34d8")
		)
		(fp_line
			(start 4.625 -5)
			(end 5.625 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75043358-1947-4b5a-9f93-f7e2f3c910f2")
		)
		(fp_line
			(start 5.625 -5)
			(end 5.625 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37f79672-5bf6-4b74-9648-17eb94770e8f")
		)
		(fp_poly
			(pts
				(xy 4.625 -5) (xy 4.625 5) (xy -4.625 5) (xy -4.625 -4) (xy -3.625 -5)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "190d91bc-93ad-45e6-b937-53f6707527bf")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "743ff2d4-173c-4e08-b34b-0138e3e452ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.925 -2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "7c007f0d-4200-491c-ae3f-0553834b99f1")
		)
		(pad "" smd roundrect
			(at -0.925 2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "61371ddf-74ee-48ff-b425-56958f3ea8eb")
		)
		(pad "" smd roundrect
			(at 3.925 -2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "402ea0d5-587b-4c86-9348-63ce088230d6")
		)
		(pad "" smd roundrect
			(at 3.925 2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "5ad45cd1-478c-42ac-99cf-663ce5b44714")
		)
		(pad "1" smd roundrect
			(at -7.65 -2.54 270)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 2 "Net-(Q2-S)")
			(pinfunction "IN")
			(pintype "power_in")
			(uuid "c0ac4bca-6826-47e0-a18b-cf3cd0665f03")
		)
		(pad "2" smd roundrect
			(at 1.5 0 270)
			(size 9.4 10.8)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.026596)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "a8142a2d-9684-4897-9b61-f8b26321fd93")
		)
		(pad "3" smd roundrect
			(at -7.65 2.54 270)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 3 "+6V")
			(pinfunction "OUT")
			(pintype "power_out")
			(uuid "6223a328-150a-4198-9f8f-b70678dc6df5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-263-2.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(uuid "3517ece5-3fd5-45e4-854e-30797eec76e3")
		(at 161.8 69.65 -90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U3"
			(at 0 -4.5 90)
			(layer "F.SilkS")
			(uuid "f00bca50-8dcf-4d28-92ef-25f14e38882c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "AZ1117-3.3"
			(at 0 4.5 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "926fe95a-a4ff-4be1-9de9-fc0223639398")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "478ce034-f25c-4718-995e-bda7b90b7d22")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 3.3V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "592ee943-82a7-42fd-8d46-88752f73ba1f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?223* SOT?89* TO?220* TO?252* TO?263*")
		(path "/72188d92-2580-438b-9ee9-b12fe3d4b97a")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.85 3.41)
			(end 1.91 3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0c62870-2343-4315-811c-449c194de6fb")
		)
		(fp_line
			(start 1.91 3.41)
			(end 1.91 2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3db44b95-b837-4ed7-ad53-6869409a93b3")
		)
		(fp_line
			(start -1.85 -3.41)
			(end 1.91 -3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd73bc3d-9f05-4d12-8252-5f498ba67cac")
		)
		(fp_line
			(start 1.91 -3.41)
			(end 1.91 -2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b205c58-47ca-4767-9786-1e80040550db")
		)
		(fp_poly
			(pts
				(xy -3.13 -3.31) (xy -3.37 -3.64) (xy -2.89 -3.64) (xy -3.13 -3.31)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "7fed5a32-75c2-42b9-ab17-038738d6d1c2")
		)
		(fp_line
			(start -4.4 3.6)
			(end 4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbd6490c-d253-4ec0-9aa3-ac57f5fdabce")
		)
		(fp_line
			(start 4.4 3.6)
			(end 4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04bbde13-8dec-4f17-ad8d-cfaac3713add")
		)
		(fp_line
			(start -4.4 -3.6)
			(end -4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f4738b4-b943-4205-94b9-7d3625955fc2")
		)
		(fp_line
			(start 4.4 -3.6)
			(end -4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "182fb891-cb79-4b0f-8210-2f63716ba311")
		)
		(fp_line
			(start -1.85 3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "66d18813-c076-467b-83f1-7c6cb53869be")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aba398a9-7d6b-469d-ada0-f9aa2bf4d099")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -0.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f1c0be4-97ae-4428-8952-eb1057d5844a")
		)
		(fp_line
			(start -0.85 -3.35)
			(end 1.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dafe4529-66ec-4dd6-804d-1e8ca27490e8")
		)
		(fp_line
			(start 1.85 -3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c225cc2-6740-4002-b356-27f7c65059de")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f834c4b8-2b31-4c3e-bd57-2a58a453a7c6")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "ebc32e97-39e2-4d8d-b8a4-c511a1741ed8")
		)
		(pad "2" smd roundrect
			(at -3.15 0 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "5670278c-8075-43be-9931-69e0201176f5")
		)
		(pad "2" smd roundrect
			(at 3.15 0 270)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "51ca8a2e-67b2-4339-a443-19f033d1b252")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "d9134b32-82c9-41ed-8f5e-69480556b26a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "466e19e0-091d-404d-b902-5ea0f6dee615")
		(at 142 42)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "301dcba8-f284-4f60-9b96-530eabb9cf3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" ".33u"
			(at 0 1.85 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a9a9e18-5e35-4072-84e0-dcd4ac9e9295")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa495882-c355-41cb-8cf3-0baade392087")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "05bc350a-b399-4226-9201-17b6ddcd81cd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a149f347-a8d1-4d59-a19e-f94f67ee342c")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4703a74-f295-4827-bff8-e24c683a2c7c")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b9f5ea9-2d56-47c0-890e-9cee85a38b57")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "45e99a3f-550f-4cc1-8ae9-df27fda407fe")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e1a06f38-0235-4fb7-882b-e5b8f6d36b56")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80209c07-e2e5-4816-aec6-315956a9498b")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c157c378-94ee-4a3c-be66-7b2e8e39ff1e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d99f434-88c7-4575-ac3e-f3d14f25accc")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11718b16-2937-48fa-8334-8264c3462ee9")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e45461e5-80c2-40d0-bb9b-27b883737647")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dcc2dc15-289e-4f37-a99c-c60d6e7c2742")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3b03fc10-e491-4fa9-b17a-42e5ac338b65")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "+6V")
			(pintype "passive")
			(uuid "b8b8ed85-12d0-4a48-b511-5d2f6594260a")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(uuid "981da7c6-2d17-4c4c-8939-c89fc7cc44f2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TO-263-2"
		(layer "F.Cu")
		(uuid "4bba009e-f709-45e2-bbb9-44e0be07520b")
		(at 158.275 53.575 -90)
		(descr "TO-263/D2PAK/DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
		(tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
		(property "Reference" "U2"
			(at 0 -6.65 90)
			(layer "F.SilkS")
			(uuid "c5613f0f-ba25-4d13-a50f-7ece4d70f500")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "L7806"
			(at 0 6.65 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7fa9209c-773e-4086-bd8a-7a1e416f45a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf5ab76e-3238-474d-a3d5-2e02fa756bb9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 6V, TO-220/TO-263/TO-252"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "dbb098a3-4be0-421c-992d-4dfcc99e4a95")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(path "/be0a7386-6c8c-4e9a-ba0e-d77ab579ea32")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.825 5.2)
			(end -4.825 3.39)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa77613c-8866-4acc-b221-0b91a9ba0f78")
		)
		(fp_line
			(start -3.46 5.2)
			(end -4.825 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f677aeb-df16-44d9-8dfd-8c1049226b33")
		)
		(fp_line
			(start -4.825 -5.2)
			(end -4.825 -3.39)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0dfabf0-298f-4631-9ab5-775a7a153135")
		)
		(fp_line
			(start -3.46 -5.2)
			(end -4.825 -5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96d12ff6-5cf6-402f-894d-7b3f92cecf88")
		)
		(fp_poly
			(pts
				(xy -7.65 -3.35) (xy -7.99 -3.82) (xy -7.31 -3.82)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "d6628e64-0bcb-492a-aa64-4c2f1a8152e1")
		)
		(fp_rect
			(start -10.2 -5.65)
			(end 6.45 5.65)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "cf79ac3b-f93e-4779-8c71-f6339ec7e38e")
		)
		(fp_line
			(start 5.625 5)
			(end 4.625 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ce95129-a7a5-4098-b0c1-6f46e7bf1d07")
		)
		(fp_line
			(start -9.325 3.04)
			(end -4.625 3.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74217e25-b1a9-4cf3-a43f-5b296bb1194a")
		)
		(fp_line
			(start -9.325 2.04)
			(end -9.325 3.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce2d1b4c-f753-4bc9-878c-08bb9a9f5e35")
		)
		(fp_line
			(start -4.625 2.04)
			(end -9.325 2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cd1f29c-d2ba-44bb-905d-7e4333c3cc49")
		)
		(fp_line
			(start -9.325 -2.04)
			(end -4.625 -2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "377fb9fb-7ee2-4e25-8f48-0d6f632a5fd6")
		)
		(fp_line
			(start -9.325 -3.04)
			(end -9.325 -2.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2578df4a-3417-4c09-8936-f0795d4bec61")
		)
		(fp_line
			(start -4.625 -3.04)
			(end -9.325 -3.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5c5fddd-04d2-4e93-8513-3f7583ff2cd1")
		)
		(fp_line
			(start 4.625 -5)
			(end 5.625 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "942f6e59-cd70-4625-b9dd-ca20305258b7")
		)
		(fp_line
			(start 5.625 -5)
			(end 5.625 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8abaa1eb-af15-4d0a-b938-536e9dade7a5")
		)
		(fp_poly
			(pts
				(xy 4.625 -5) (xy 4.625 5) (xy -4.625 5) (xy -4.625 -4) (xy -3.625 -5)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "2155ccea-4e98-48ee-96c6-bd1f7029d6b1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "9949735f-ac26-4e9a-82a9-4f5014fb8529")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.925 -2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "3bd74575-1e81-47ed-8e22-59ae70aa8a22")
		)
		(pad "" smd roundrect
			(at -0.925 2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "376a5917-7fc1-4197-a8a9-0781af67c7ec")
		)
		(pad "" smd roundrect
			(at 3.925 -2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "440a596a-ddac-4a95-aff1-21860c5a09e5")
		)
		(pad "" smd roundrect
			(at 3.925 2.775 270)
			(size 4.55 5.25)
			(layers "F.Paste")
			(roundrect_rratio 0.054945)
			(uuid "878876ae-c7f3-48cc-9c79-c6913f560d42")
		)
		(pad "1" smd roundrect
			(at -7.65 -2.54 270)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 2 "Net-(Q2-S)")
			(pinfunction "IN")
			(pintype "power_in")
			(uuid "fea9d56e-c5a3-484a-89e4-266bafc0c198")
		)
		(pad "2" smd roundrect
			(at 1.5 0 270)
			(size 9.4 10.8)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.026596)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "80680ef2-5138-4893-949a-985c7cec96a6")
		)
		(pad "3" smd roundrect
			(at -7.65 2.54 270)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 3 "+6V")
			(pinfunction "OUT")
			(pintype "power_out")
			(uuid "f9daf59d-0ecc-4757-9ae9-e6a4eef3b2b2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-263-2.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "5db7bacc-3569-4d46-befe-fe76b5d6b192")
		(at 143.95 69.5625 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.83 90)
			(layer "F.SilkS")
			(uuid "ad7113a7-8766-4eb4-ae65-2fc6352083fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.83 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b01bee6f-27eb-4687-9141-baa82c25a2db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f5b3f69f-b13b-44de-b77a-8e1c07687735")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "487e71c9-40af-425c-8345-eee2ab5a8bd5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d6b22495-79e5-449e-81dd-4f6bce126c42")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da9aef95-8b36-4528-9d7c-ff8cea496d55")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c36898bf-9147-4762-9329-d205258770e2")
		)
		(fp_line
			(start 2.28 -1.13)
			(end 2.28 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1258c412-3c07-435e-84ea-c0385002cf12")
		)
		(fp_line
			(start -2.28 -1.13)
			(end 2.28 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33985461-ea41-4559-8683-783df29d5ee3")
		)
		(fp_line
			(start 2.28 1.13)
			(end -2.28 1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5ff15c7-2a3d-48cb-8b1e-79ee9d386261")
		)
		(fp_line
			(start -2.28 1.13)
			(end -2.28 -1.13)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acdb9a1e-1df7-4f98-a178-53d36c5d2409")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31e5f9aa-065e-4d1b-a40a-8ed5ede29aaa")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "216b14ed-5f8f-4cda-b47c-bc26bb5ddb3b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cae5edf6-e9c7-4bfb-bfd5-bf73c5e79ff3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59b57ab5-5ac7-4ca2-b82a-a33b5e039df5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "4f9687b8-3daa-4ceb-8036-d88bec9f9ea3")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 7 "VBUS")
			(pintype "passive")
			(uuid "b1e1ca47-14c8-42f4-919d-8b12eae677cb")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bfa2108d-c46f-4586-a986-02c150b13867")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "7be5bb3f-5a73-4ed9-a244-cb78d88b4d9a")
		(at 150 47 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -3 0 180)
			(layer "F.SilkS")
			(uuid "318dbd85-6ec4-4fbc-bde0-85eeef9dc613")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" ".33u"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "1297600b-f8bd-4e4f-9dc1-17659d8d1c1a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2d05fc2-fae4-490f-90f0-c300c4b8ea9c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "74eebd07-0b90-4187-b813-89c69bb4f7c1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/daa7595a-76e8-42c7-9dcc-7320974f7431")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10606671-4938-4ab4-a60a-4db3eecd26a9")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9cf2353d-7cf3-4e52-bb84-4bd246c74634")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0246d44a-a2f2-4c97-b100-6252f08cf750")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "141163eb-2e1d-4bf1-868e-0c7d1af5c87f")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f2ea6886-10aa-4aaf-ad74-6ed0b1610315")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "208cc41c-cf99-4a71-98cb-12ace69cd973")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18e56b26-492a-4b7a-ab0b-0b46ecea025c")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab744316-8703-4094-8c05-45e1ff1f6a20")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0707f445-7851-46d9-b6ce-aab12aa22b69")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e0f0692-765a-4539-98d4-9643bce60f9a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "fb0b82e1-a6c3-4bb9-b697-7e1238eb0426")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "Net-(Q2-S)")
			(pintype "passive")
			(uuid "72822a9f-e053-42fc-9b06-c29b31ea97f3")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6fe442b1-e1c4-46df-a233-e30a9edcaa28")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "a1c51d0a-cd80-4bd6-9957-b01f81ab4eda")
		(at 152.95 63.1875 -90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "99835f0b-bdfe-4ced-9d85-66a60a9a4fdb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SSM3J328R,LF"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f174946d-a572-47e2-babe-075042d8d920")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "966d7ab2-6bf2-4011-9cac-77dd2543fc82")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a801461-5531-41af-a364-55fd7729da78")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PMOS"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0b38a49-1a95-4658-8d20-4f2f45c37364")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef37cda4-282d-48dc-b012-dd800b0d9ee7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9b550b3e-6dcd-4c46-81f0-b0eea4f63ace")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/8489bd15-4c6c-4e6d-b841-c55757b76d44")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.76 1.56)
			(end -0.76 1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07b38b6e-3d3a-4f88-89d2-06980c9b367c")
		)
		(fp_line
			(start 0.76 1.56)
			(end -0.76 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3135a170-6185-4209-a8bd-99b20d807fcf")
		)
		(fp_line
			(start 0.76 0.56)
			(end 0.76 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ff7897b-7513-492c-8700-6e961a743b61")
		)
		(fp_line
			(start -0.76 0.39)
			(end -0.76 -0.39)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c592b36-b1f0-4900-b313-8cdb04c2acf2")
		)
		(fp_line
			(start -0.76 -1.51)
			(end -0.76 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3be6a8f1-cd25-4040-bf5f-3bcf070bf312")
		)
		(fp_line
			(start -0.76 -1.56)
			(end 0.76 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16ecec6f-3f72-4f52-9e09-15f294b9dea3")
		)
		(fp_line
			(start 0.76 -1.56)
			(end 0.76 -0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3df5db5c-b1ba-4cab-9e04-050bd644d48a")
		)
		(fp_poly
			(pts
				(xy -1.3 -0.38) (xy -1.06 -0.05) (xy -1.54 -0.05)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "0b38ce51-c155-4fd9-a9c8-b749d52069fb")
		)
		(fp_line
			(start -0.9 1.7)
			(end -0.9 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a2c7d47e-3149-4976-bdcf-f993e623c753")
		)
		(fp_line
			(start 0.9 1.7)
			(end -0.9 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5597512-c225-4730-b057-18970e03f6a2")
		)
		(fp_line
			(start -1.93 1.5)
			(end -1.93 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a888cbb8-986a-42be-af9f-f83316147721")
		)
		(fp_line
			(start -0.9 1.5)
			(end -1.93 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "000addf1-aec8-4199-aea1-497377c2da29")
		)
		(fp_line
			(start 0.9 0.55)
			(end 0.9 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af4d1e4c-6351-4acb-b683-fd65a441ab00")
		)
		(fp_line
			(start 1.93 0.55)
			(end 0.9 0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "65a1ba65-523d-4b64-bbf2-56655d137b47")
		)
		(fp_line
			(start 0.9 -0.55)
			(end 1.93 -0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff02053a-21a6-4461-8256-f8ebeda8f638")
		)
		(fp_line
			(start 1.93 -0.55)
			(end 1.93 0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "843b3c93-532b-44af-b4fa-136e750b04ea")
		)
		(fp_line
			(start -1.93 -1.5)
			(end -0.9 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df13fdb3-3e9a-4f0f-a93e-e3dc45287248")
		)
		(fp_line
			(start -0.9 -1.5)
			(end -0.9 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c937dd3-b8a3-45f0-b063-6167596615ce")
		)
		(fp_line
			(start -0.9 -1.7)
			(end 0.9 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43718b75-ed39-43ea-b89e-f4d061d2455c")
		)
		(fp_line
			(start 0.9 -1.7)
			(end 0.9 -0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41952158-cf74-4d98-aa62-d1a55103b1d1")
		)
		(fp_poly
			(pts
				(xy -0.65 -1.125) (xy -0.65 1.45) (xy 0.65 1.45) (xy 0.65 -1.45) (xy -0.325 -1.45)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "92341474-d1a3-4bff-9fe9-e4ded32b72ad")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "91480328-70da-4309-8a3e-35b7fdfc552e")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.11)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+BATT")
			(pinfunction "D")
			(pintype "passive")
			(uuid "d63671e1-d69d-4abf-91bb-28db72006c08")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "VBUS")
			(pinfunction "G")
			(pintype "input")
			(uuid "3291549e-6db8-4ca7-922e-595a7f80acb8")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pinfunction "S")
			(pintype "passive")
			(uuid "1b3aa9fe-f3d3-4944-a705-84a076a5a9e1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "a33f10ea-e0b7-4d1a-a91a-18b92a8c756c")
		(at 165.5 47 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 3 0 180)
			(layer "F.SilkS")
			(uuid "d62cb11b-45bb-417c-8c85-ec5e639a573b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" ".33u"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7866aea8-2f9d-49c9-8155-1b8012088fb0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "98fb71b6-9397-48cd-be00-a8f57c05fb06")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b34f4c44-7301-4def-8016-468bf53b4600")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b5ee3f34-4d7e-4f76-98ef-9462a77f44ad")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f622a86e-980e-473f-bdf7-6273dfd22d04")
		)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9cabf43f-dc24-4a87-851d-7ae3819250f9")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94bfdcd8-e582-40d2-a406-7f194d800a6f")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50d3c78c-13ff-4006-866a-93103fce540d")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24980fc4-fde9-488b-bf19-545a65f24cfc")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "be906aa0-040f-4272-9b62-05ddd58b1363")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c43db9d7-4e04-41fb-bdc4-e59a5a1dd026")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d37173a7-67fb-411c-ae86-eec57133f4dd")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b23e89d8-f3ac-4ac0-8e7d-922018eb9d76")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "068ad681-e991-4032-b2e9-43f363400f54")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "8aaf8e44-6e70-4bb3-8733-61d6cebc73d6")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "Net-(Q2-S)")
			(pintype "passive")
			(uuid "76ab779b-e495-4f61-9b03-a47da2bbad14")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6b0459f0-f3e9-4be1-a5a2-e21e56b178a6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "a73fd9b5-5fb4-4be3-85fb-7bfda4615aa9")
		(at 161.8 62.825 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 2 90)
			(layer "F.SilkS")
			(uuid "4e19fae2-f195-44a9-9569-4f445dca93d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22u"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "482779a0-f2f9-4163-87c9-f3392d1e14d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f622b07-a053-47c8-acab-88913083cda7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2c65589-ebc9-4ac5-b1c8-3589eb8518eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/ff13d6df-7f41-49a1-9d3d-f662335654bd")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58c57449-d603-4e2a-b4d9-f2f54260ffd8")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d29c108-d52c-498b-b166-4ac7533a97a2")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7e1031e-f040-4940-869d-d065b562bd55")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d268958-74d2-4a49-bdb8-8ec88d93774b")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4757e2d7-6acb-4a42-b081-afdac8a957e2")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28103111-6531-4edd-9292-80a307cff3de")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9bd4f5a-c225-4e5c-bbed-53fb3af6ea66")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd9b9633-756b-4f0a-a7d9-1694389e598e")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0daa763-b970-4614-901b-2acd8fa3fc3c")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4b12e4d-e5c1-4046-a43c-7a5ed15d5bdb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "567cb88f-8daf-44f1-b137-073e3d4e6530")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 5 "+3.3V")
			(pintype "passive")
			(uuid "7cb75796-dc5f-4b21-8de0-c0903b8f8a81")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9baa4a6a-3030-4bdf-942e-94b6dcd7d5c8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-128"
		(layer "F.Cu")
		(uuid "ad381caf-f3bb-4d47-aff8-e49334cf801b")
		(at 147.95 68.5625 -90)
		(descr "D_SOD-128 (CFP5 SlimSMAW), https://assets.nexperia.com/documents/outline-drawing/SOD128.pdf")
		(tags "D_SOD-128")
		(property "Reference" "D2"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(uuid "bc7d2a44-1e40-4781-a783-86b9e45225f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PMEG10030ELPX"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "162a8c12-39be-4e34-a1ba-ff3ff93385ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3bc1bb8f-0db6-45f8-8aef-68dad4297122")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Schottky diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "60436788-00d0-44a3-a620-acd9bf30fdb9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/4ed141a5-6d38-4679-81d5-0472e27083d3")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.16 1.36)
			(end 1.9 1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa988f0a-fd36-4080-b4f3-6fa06e00ddb8")
		)
		(fp_line
			(start -3.16 -1.36)
			(end -3.16 1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8beed988-2de3-4bdd-941a-2751189eb093")
		)
		(fp_line
			(start -3.16 -1.36)
			(end 1.9 -1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10826974-4ea7-45a0-8e35-153feb501e86")
		)
		(fp_line
			(start 3.15 1.5)
			(end -3.15 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68346068-a298-46fc-be55-9d7b0d74c4b0")
		)
		(fp_line
			(start -3.15 -1.5)
			(end -3.15 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a64d3897-e68e-4ef7-ae68-1dd4ecf8af41")
		)
		(fp_line
			(start -3.15 -1.5)
			(end 3.15 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b6130b2b-0e37-462b-8821-b948d16626ce")
		)
		(fp_line
			(start 3.15 -1.5)
			(end 3.15 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89bb81f2-0253-4705-9ee5-288cde9e6f83")
		)
		(fp_line
			(start -1.9 1.25)
			(end -1.9 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "658178b1-961c-4b01-8b74-fb9d30ab7932")
		)
		(fp_line
			(start 1.9 1.25)
			(end -1.9 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1add5bf4-0082-44fb-9228-64d14407eaa4")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7e1bfac-1e46-487a-849e-4f9f044d3778")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1adec796-9ddc-4fe8-bbfb-76e123464a73")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17f06a2d-3180-4a81-a4dc-9a4a7b8808f0")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5595f646-dbb3-4f00-9d7b-5767649caf34")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91757723-5c3e-4e4b-a622-637ebba4435b")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e613c406-da32-44ff-b453-c960153ea71f")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c34d4637-160a-4604-8126-1574813b29c3")
		)
		(fp_line
			(start -1.9 -1.25)
			(end 1.9 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd7a567c-921c-4228-baaa-d803fc71a56c")
		)
		(fp_line
			(start 1.9 -1.25)
			(end 1.9 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ec812c0-34c8-430f-be2e-065d5119b5bd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
			(uuid "45a77fbb-0450-4640-b340-ad269f51a7eb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.2 0 270)
			(size 1.4 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1785714286)
			(net 3 "+6V")
			(pinfunction "K")
			(pintype "passive")
			(uuid "cd27a475-40bc-4fc5-9cb7-8394d1f76499")
		)
		(pad "2" smd roundrect
			(at 2.2 0 270)
			(size 1.4 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1785714286)
			(net 7 "VBUS")
			(pinfunction "A")
			(pintype "passive")
			(uuid "bda8c64b-1de2-4f75-92c6-4bce0ef2e962")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-128.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "bd4911ed-c3dd-4cbd-9dd1-f7efc27310a8")
		(at 147.95 63.0625 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "30de45f9-aa4f-40bf-8c8c-cc143c7b75bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SSM3J328R,LF"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7712f1ce-5260-400c-b43b-ff9a367d2899")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "3888db3a-db6c-4ee2-8778-b6f45f0b7869")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "eb7a661c-e29b-4ba1-b1fd-51aed5071813")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e833a6db-7ede-4b6f-9740-f86295b78510")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "263dac25-0ffb-43b4-8897-1b3bb736ca31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "267b635c-f16d-4df3-b1f0-c05b84d84f59")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/abf68102-86c1-4bb0-a97c-236c7e6dc156")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.76 -1.56)
			(end 0.76 -0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a68844b-6442-48af-9193-d0380a5b855f")
		)
		(fp_line
			(start -0.76 -1.56)
			(end 0.76 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3523f05b-19e2-4018-bc6b-562f95a36f77")
		)
		(fp_line
			(start -0.76 -1.51)
			(end -0.76 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d41e30f-9c30-4003-a477-561a55a42487")
		)
		(fp_line
			(start -0.76 0.39)
			(end -0.76 -0.39)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b656bf6b-ece3-4f12-bf83-917bac25138b")
		)
		(fp_line
			(start 0.76 0.56)
			(end 0.76 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ed787d2-15b5-488d-aceb-307912dac591")
		)
		(fp_line
			(start 0.76 1.56)
			(end -0.76 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86448726-2d63-4448-9b8f-6f460c4be36b")
		)
		(fp_line
			(start -0.76 1.56)
			(end -0.76 1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15319d04-61b7-483d-80ab-279deb2f3e91")
		)
		(fp_poly
			(pts
				(xy -1.3 -0.38) (xy -1.06 -0.05) (xy -1.54 -0.05)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "84bee4ae-b9b4-4dbf-818f-23fd530a28db")
		)
		(fp_line
			(start 0.9 -1.7)
			(end 0.9 -0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19fc1572-3811-490b-ad14-ebcc142bd2e4")
		)
		(fp_line
			(start -0.9 -1.7)
			(end 0.9 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "48b337a2-3023-4a56-9058-a8b653c70cb4")
		)
		(fp_line
			(start -0.9 -1.5)
			(end -0.9 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "656e0a38-e3da-4e0f-bf97-adbfae072ae3")
		)
		(fp_line
			(start -1.93 -1.5)
			(end -0.9 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "be9364db-9f30-4ae3-9954-1f4142b1ae2a")
		)
		(fp_line
			(start 1.93 -0.55)
			(end 1.93 0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e769ab57-1eac-4327-bf2b-c13b50395a78")
		)
		(fp_line
			(start 0.9 -0.55)
			(end 1.93 -0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "710df9bf-6d50-44ce-8d46-0e364324df94")
		)
		(fp_line
			(start 1.93 0.55)
			(end 0.9 0.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f53fa7d-e374-4e28-8d99-d7cda7fef56c")
		)
		(fp_line
			(start 0.9 0.55)
			(end 0.9 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3aa7a59b-eb3c-4ffb-93a6-c5a9e083f015")
		)
		(fp_line
			(start -0.9 1.5)
			(end -1.93 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05365021-b7ca-4f16-a0bf-35cd3e248427")
		)
		(fp_line
			(start -1.93 1.5)
			(end -1.93 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a1def78a-aa51-4576-8efd-b9e033f358ea")
		)
		(fp_line
			(start 0.9 1.7)
			(end -0.9 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71428e52-7d37-4dd4-ae1f-7c9a75de2c19")
		)
		(fp_line
			(start -0.9 1.7)
			(end -0.9 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21eb5d14-9e29-4b18-b84e-7789a4f3788c")
		)
		(fp_poly
			(pts
				(xy -0.65 -1.125) (xy -0.65 1.45) (xy 0.65 1.45) (xy 0.65 -1.45) (xy -0.325 -1.45)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "6b8bc0f3-6117-486a-864f-93993d7bd1e4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f29e81af-6cc6-4217-9b24-9dfa487a993a")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.11)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pinfunction "D")
			(pintype "passive")
			(uuid "25cd93cb-6229-4113-ad2a-345a09f4b218")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "VBUS")
			(pinfunction "G")
			(pintype "input")
			(uuid "323d31c7-318d-4cc5-9cac-14326266dbae")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(Q2-S)")
			(pinfunction "S")
			(pintype "passive")
			(uuid "7ee64018-b37b-46f9-b089-358dc2a6f6b2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-128"
		(layer "F.Cu")
		(uuid "f3ae60e4-289c-40f4-8847-b29dd92035fa")
		(at 152.95 68.5625 -90)
		(descr "D_SOD-128 (CFP5 SlimSMAW), https://assets.nexperia.com/documents/outline-drawing/SOD128.pdf")
		(tags "D_SOD-128")
		(property "Reference" "D1"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(uuid "5534fa10-fe38-4125-8bc2-d6fb5d352667")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PMEG10030ELPX"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ba30b494-6d10-44ca-ad37-d94090642b09")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0f824ec8-f211-43df-a24e-be4f6efa8d11")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Schottky diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e577abfa-2d57-4c72-9033-61b424136de2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/bff1059a-d811-4a2a-b1ad-67ab92d3aad8")
		(sheetname "/")
		(sheetfile "power-subsystem-new.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.16 1.36)
			(end 1.9 1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d8adf2e-cfe9-4079-8fdd-2f1f304c681e")
		)
		(fp_line
			(start -3.16 -1.36)
			(end -3.16 1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b91d5c0-5931-4c8e-a356-a1a27066fdb0")
		)
		(fp_line
			(start -3.16 -1.36)
			(end 1.9 -1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3347ffb5-8865-44f6-a3a2-cdc408e03e40")
		)
		(fp_line
			(start 3.15 1.5)
			(end -3.15 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5496ba89-4a34-43d8-8612-810cd785d7ef")
		)
		(fp_line
			(start -3.15 -1.5)
			(end -3.15 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6d802049-5a89-4dee-8bfb-bcd5f22f296a")
		)
		(fp_line
			(start -3.15 -1.5)
			(end 3.15 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3376a13e-2e0f-49fb-aacf-bc36ec2d7ce0")
		)
		(fp_line
			(start 3.15 -1.5)
			(end 3.15 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b5e1ba9-9749-4cb1-95dc-c546be6d5d1b")
		)
		(fp_line
			(start -1.9 1.25)
			(end -1.9 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03a330c9-53f4-46c4-a1f7-b27e8866e5df")
		)
		(fp_line
			(start 1.9 1.25)
			(end -1.9 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef9c802e-894a-418f-9ca7-afac96084f18")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9139e75-37a5-4254-b2b8-3bd4f69596fd")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3e0743a-5a4e-4737-8682-112cbd4b12f2")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32c58446-91d7-4882-a4e6-935387aaf2d2")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7f86fc4-bd70-4308-8b86-6bbb5e646499")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00362cb0-833f-4cf7-bf2c-96543825d635")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1409a0da-8dcb-4b70-9bb3-bfaab43b8f7e")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a90dcb3c-3cff-49d4-ae6c-586dc648bd0f")
		)
		(fp_line
			(start -1.9 -1.25)
			(end 1.9 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "217cb90a-f588-4b68-86ef-e1c01e51267f")
		)
		(fp_line
			(start 1.9 -1.25)
			(end 1.9 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17ce738a-b0df-4ebf-8a6d-10fd4b85c9dc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
			(uuid "8e296f00-dc8e-4d20-9d8d-cbaaffd5f24f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.2 0 270)
			(size 1.4 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1785714286)
			(net 4 "VDD")
			(pinfunction "K")
			(pintype "passive")
			(uuid "700f3cdb-98e9-4f37-acd8-de61f3be7a31")
		)
		(pad "2" smd roundrect
			(at 2.2 0 270)
			(size 1.4 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1785714286)
			(net 7 "VBUS")
			(pinfunction "A")
			(pintype "passive")
			(uuid "50d6b116-a71f-4531-9a82-70d28a98f513")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-128.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 135.5 39)
		(end 167.5 75)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "c6d617b1-e1d9-41f6-b3dc-f440d9a0731d")
	)
	(segment
		(start 141.599 70.3339)
		(end 141.599 71.6661)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "0ed98ab0-4fde-46f7-bcdc-8fb87e1202f6")
	)
	(segment
		(start 144.0339 74.101)
		(end 163.899 74.101)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "13bfec7b-65a3-4f5f-bbd5-1b47eea2c8c4")
	)
	(segment
		(start 154.884 41.37984)
		(end 155.46484 40.799)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "14d2f245-2b9a-402d-8ee3-b3729d7c58be")
	)
	(segment
		(start 160.27984 48.526)
		(end 165.449 48.526)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "1b236e8e-1f92-407b-9f31-431c7b33cc09")
	)
	(segment
		(start 157.774 40.799)
		(end 158.975 42)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "22847656-8d8e-4c95-a820-a96cfc601570")
	)
	(segment
		(start 158.275 60.275)
		(end 158.275 55.075)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "41b3c248-3a8f-4ba4-8576-1dbd4298405e")
	)
	(segment
		(start 161.75 61.3)
		(end 161.8 61.35)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "43bfb4f0-719e-4769-8453-5e4489588d50")
	)
	(segment
		(start 155.46484 40.799)
		(end 157.774 40.799)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "4476b439-60fa-45ac-acda-2f67809ea74c")
	)
	(segment
		(start 159.3 61.3)
		(end 158.275 60.275)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "4f11d0b3-2504-4c8a-9810-3c418c7289e6")
	)
	(segment
		(start 154.884 45.35216)
		(end 154.884 41.37984)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "4f9eff42-4d0f-46d0-92f3-b4468b47d55d")
	)
	(segment
		(start 141.599 71.6661)
		(end 144.0339 74.101)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "64b5409c-aae5-4acf-b27c-729f0599a4d7")
	)
	(segment
		(start 164.1 66.5)
		(end 164.1 63.65)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "6a419140-42fa-43a5-ad71-6fb800902cea")
	)
	(segment
		(start 143.475 42)
		(end 143.475 54.635)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "72e21051-4cec-4e1a-b352-beb271718991")
	)
	(segment
		(start 164.1 63.65)
		(end 161.8 61.35)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "74f312c3-8bcd-407f-a4f3-8e169f2b01a9")
	)
	(segment
		(start 146.475 42)
		(end 143.475 42)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "7b5fd19f-f4b5-420e-8c97-7f70b57ef184")
	)
	(segment
		(start 158.975 42)
		(end 158.975 47.22116)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "88be5af9-ad49-464e-9263-bef2c13c6d76")
	)
	(segment
		(start 164.5 66.9)
		(end 164.1 66.5)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "8fb894f3-3895-4696-8e69-1f188301567a")
	)
	(segment
		(start 145.08616 55.15)
		(end 154.884 45.35216)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "97fe559c-ceb6-4a3a-9551-2dfb1e1fb7a6")
	)
	(segment
		(start 164.5 73.5)
		(end 164.5 66.9)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "9ffd1a35-fd84-4243-91e4-283b8df37915")
	)
	(segment
		(start 159.3 61.3)
		(end 161.75 61.3)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "a1578d9e-273f-4ff2-9a03-9abd7e2655f3")
	)
	(segment
		(start 143.95 68.1)
		(end 143.8329 68.1)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "a42d7406-5c2a-4c93-9c42-fdaf9138f2fe")
	)
	(segment
		(start 142.96 55.15)
		(end 145.08616 55.15)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "a4aa1921-16bd-43cd-b279-9bbc76f8ef19")
	)
	(segment
		(start 163.899 74.101)
		(end 164.5 73.5)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "b2921a31-5f31-4c1d-87f5-52ad8a65cce5")
	)
	(segment
		(start 143.475 54.635)
		(end 142.96 55.15)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "b9b6b26a-66e5-4568-9c47-ddd962e9bd88")
	)
	(segment
		(start 158.975 47.22116)
		(end 160.27984 48.526)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "c377cc39-7c1d-400f-9366-b66caed1c9d6")
	)
	(segment
		(start 150 45.525)
		(end 146.475 42)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "c90bc2a2-7d85-4c46-811a-92d7dcbf715f")
	)
	(segment
		(start 158.9 55.075)
		(end 165.5 48.475)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "d33582ff-41e7-459b-bf40-e1b435cf9f16")
	)
	(segment
		(start 143.8329 68.1)
		(end 141.599 70.3339)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "d787e399-bbd6-4c6e-a083-787dc2c00c0f")
	)
	(segment
		(start 158.275 55.075)
		(end 158.9 55.075)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "f0fa55d7-435b-4185-a59c-1d440a3ca734")
	)
	(segment
		(start 165.449 48.526)
		(end 165.5 48.475)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "f6364fce-8124-4e57-8945-c37a1a4917e2")
	)
	(segment
		(start 136.599 44.16484)
		(end 139.96484 40.799)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "14a5ee20-71d3-4886-b251-0a07eecf8ede")
	)
	(segment
		(start 152.5 41)
		(end 152.5 44.5)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "3868ec59-0cd4-4191-b99f-782363ee8edb")
	)
	(segment
		(start 165.1 45.925)
		(end 165.5 45.525)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "413ec418-b45c-4d7c-9f55-5104019dd054")
	)
	(segment
		(start 152.5 45.975)
		(end 150 48.475)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "45b6cb5e-d2dd-4734-97d2-ff074b60040f")
	)
	(segment
		(start 160.815 45.925)
		(end 165.1 45.925)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "4756cb77-95a8-4a95-8a85-3dc56c4e8050")
	)
	(segment
		(start 148.799 40.799)
		(end 152.5 44.5)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "4bbb6ffa-ff28-4ef3-acde-c24828657de8")
	)
	(segment
		(start 147.975 48.475)
		(end 145.5 46)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "54fc0175-dd42-4ba2-b446-ac8cea461c59")
	)
	(segment
		(start 136.599 60.1661)
		(end 136.599 44.16484)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "78d7080a-53ec-470f-8e8a-bb0a650fc0c9")
	)
	(segment
		(start 165.5 43.5)
		(end 162 40)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "a55d195a-56de-4312-ae8a-1cb865b63331")
	)
	(segment
		(start 139.96484 40.799)
		(end 148.799 40.799)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "a6bd1498-c38f-44ed-8ea5-fa68914bbabf")
	)
	(segment
		(start 150 48.475)
		(end 147.975 48.475)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "ab003ebc-5996-4484-9d06-c5ab64fef070")
	)
	(segment
		(start 165.5 45.525)
		(end 165.5 43.5)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "b6662b6f-94f2-4229-a30f-152421b21f1f")
	)
	(segment
		(start 162 40)
		(end 153.5 40)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "bc26cbed-a414-408f-8c1d-6da664dbaec4")
	)
	(segment
		(start 138.5579 62.125)
		(end 136.599 60.1661)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "c04f4427-e2cf-4efa-ac2a-e655e70895a8")
	)
	(segment
		(start 153.5 40)
		(end 152.5 41)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "d9ec3786-9b30-4df2-b33b-745352c02dde")
	)
	(segment
		(start 147.95 62.125)
		(end 138.5579 62.125)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "ea3a9c3e-98c9-42ae-838d-1d951bbe4a02")
	)
	(segment
		(start 152.5 44.5)
		(end 152.5 45.975)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "ed287329-ca65-4f6c-af2f-1fa74afab61f")
	)
	(segment
		(start 147.95 63.504468)
		(end 148.661 62.793468)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "08bba384-7608-4020-89bc-c608ea0ccaf3")
	)
	(segment
		(start 137 49.42)
		(end 137 60)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "45fd879f-c54a-4d12-aef9-ea18d296e6a8")
	)
	(segment
		(start 156.025 45.635)
		(end 155.735 45.925)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "4f9ae50f-4be2-4d36-962b-9f4abfc155a2")
	)
	(segment
		(start 148.661 62.793468)
		(end 148.661 59.83516)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "7b76b1da-7c7a-401b-b6b0-c319b486acde")
	)
	(segment
		(start 147.99616 60.5)
		(end 148.661 59.83516)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "92fd0d20-9b40-4159-b91f-8d13a1a7850e")
	)
	(segment
		(start 140.42 46)
		(end 137 49.42)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "952ba7b9-3440-4cde-923f-2635c0391851")
	)
	(segment
		(start 140.525 45.895)
		(end 140.42 46)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "a54c2172-a7cf-49d8-96b2-3cf0b8b04e52")
	)
	(segment
		(start 148.661 59.83516)
		(end 148.661 52.999)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "a97f5e76-8d06-4d96-928d-978844e20fe7")
	)
	(segment
		(start 148.661 52.999)
		(end 155.735 45.925)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "af734e60-08ed-473d-bdef-0058509bc1c2")
	)
	(segment
		(start 137 60)
		(end 137.5 60.5)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "c0109d7b-f5b9-46f5-a8b8-368d6a9359f9")
	)
	(segment
		(start 156.025 42)
		(end 156.025 45.635)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "cd049e50-2331-4dba-82da-90c2fcae3009")
	)
	(segment
		(start 147.95 66.3625)
		(end 147.95 63.504468)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "d87b3db7-634a-4083-824e-1f796a3e7c0f")
	)
	(segment
		(start 137.5 60.5)
		(end 147.99616 60.5)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "ef79ea72-a629-4f35-bd08-b1a364c08351")
	)
	(segment
		(start 140.525 42)
		(end 140.525 45.895)
		(width 0.2)
		(layer "F.Cu")
		(net 3)
		(uuid "fa7a7de5-3adb-4b79-8c1c-a2a350534b49")
	)
	(segment
		(start 145.5 65.5)
		(end 145.5 69)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "0ae3c523-850d-41ba-aed7-0680ee45c3ca")
	)
	(segment
		(start 147 64)
		(end 145.5 65.5)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "221e2963-ef5e-48e4-906e-a166787b8504")
	)
	(segment
		(start 145.5 69)
		(end 144.5 70)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "26ae6510-d1b0-4492-9102-592dbb839f47")
	)
	(segment
		(start 144.5 70)
		(end 142.5 70)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "3e4e899e-47e6-4a72-93fe-c3c3986f17b9")
	)
	(segment
		(start 159.3 66.3)
		(end 159.5 66.5)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "3ee67892-6e0d-4613-8676-91e682001e93")
	)
	(segment
		(start 143 72.5)
		(end 155 72.5)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "81307af7-07bf-4255-b1df-af10e7953214")
	)
	(segment
		(start 152.95 66.3625)
		(end 152.95 64.125)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "9f7cd5ca-36c3-4f65-904b-62204a52d3d6")
	)
	(segment
		(start 159.3 64.25)
		(end 159.3 66.3)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "9f85218c-a2c4-4703-998e-2beb3feca883")
	)
	(segment
		(start 159.3 64.25)
		(end 153.075 64.25)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "a242ec6f-680e-4e1e-b182-dbba745b3b63")
	)
	(segment
		(start 153.075 64.25)
		(end 152.95 64.125)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "a4f46b73-d156-4dc2-8dcc-0351bab8c849")
	)
	(segment
		(start 159.5 68)
		(end 159.5 66.5)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "a4ffd160-556c-4472-bcfe-5b325b659a18")
	)
	(segment
		(start 142 71.5)
		(end 143 72.5)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "b6cb6d68-631d-4fce-9f5a-11cac80385a4")
	)
	(segment
		(start 155 72.5)
		(end 159.5 68)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "c71bc946-f0b6-4cfa-ae5a-feeb3bac1d5a")
	)
	(segment
		(start 142.5 70)
		(end 142 70.5)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "d8eca67a-d4b4-43c0-afcb-c93004fe5fee")
	)
	(segment
		(start 142 70.5)
		(end 142 71.5)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "fe688595-f23b-46db-aec7-4998c15718e0")
	)
	(segment
		(start 161.8 72.8)
		(end 161.8 66.5)
		(width 0.2)
		(layer "F.Cu")
		(net 5)
		(uuid "0383bf79-7a47-411f-bc00-80539c189fb4")
	)
	(segment
		(start 161.8 64.3)
		(end 161.8 66.5)
		(width 0.2)
		(layer "F.Cu")
		(net 5)
		(uuid "0e1bd068-5f9a-4d9b-a3fb-8d390d4f0120")
	)
	(segment
		(start 151 70.2625)
		(end 150.5 70.7625)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "0da5fb1f-ce34-4e9a-a4af-55e134290d22")
	)
	(segment
		(start 147.6875 71.025)
		(end 147.95 70.7625)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "19f2e7d6-4936-41fe-92ec-2b0f2d93ba6c")
	)
	(segment
		(start 148.9 64)
		(end 151 66.1)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "36871335-ffc9-4fb9-a5a3-bb5e3c0d5d64")
	)
	(segment
		(start 143.95 71.025)
		(end 147.6875 71.025)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "422f2904-2b81-4fe7-a1d0-34c84b41db95")
	)
	(segment
		(start 150.65 62.25)
		(end 152 62.25)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "661a6eed-c9db-48d3-8a0a-c2ab0ba78534")
	)
	(segment
		(start 152.95 70.7625)
		(end 150.5 70.7625)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "7de4931d-2e6a-4332-a156-7b584b89eb6c")
	)
	(segment
		(start 151 66.1)
		(end 151 70.2625)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "8f248179-404a-4eee-ac8f-22da618dfb64")
	)
	(segment
		(start 150.5 70.7625)
		(end 147.95 70.7625)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "b148b826-53d4-401f-958e-2d35cf35810e")
	)
	(segment
		(start 148.9 64)
		(end 150.65 62.25)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "e590c1b0-33ae-49fd-9a99-0c8a1efdc0fa")
	)
	(embedded_fonts no)
)
