Glucometer

Team Meeting Agenda

April 2, 2015

Design Review II

System

* FSM works and instructs the user through the LCD screen
* ADC circuit generates a voltage
* LCD displays that voltage value
* Bluetooth sends the value to the app
* App receives it and displays it