(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MIC23150-SYMT-TR"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "MIC23150-SYMT-TR"
			(at 0 8.89 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" "MLF-8_MT_MCH"
			(at 0 -9.144 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "MIC23150-SYMT-TR"
			(at -0.254 -9.144 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "ki_keywords" "MIC23150-SYMT-TR"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "MLF-8_MT_MCH MLF-8_MT_MCH-M MLF-8_MT_MCH-L"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "MIC23150-SYMT-TR_0_1"
			(polyline
				(pts
					(xy -6.8707 5.08) (xy -7.9121 5.6007)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.8707 5.08) (xy -7.9121 4.5593)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.8707 2.54) (xy -7.9121 3.0607)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.8707 2.54) (xy -7.9121 2.0193)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.8707 0) (xy -7.9121 0.5207)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.8707 0) (xy -7.9121 -0.5207)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.8707 0.5207) (xy 7.9121 0)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.8707 -0.5207) (xy 7.9121 0)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.8707 -2.0193) (xy 7.9121 -2.54)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.8707 -3.0607) (xy 7.9121 -2.54)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.8707 -4.5593) (xy 7.9121 -5.08)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.8707 -5.6007) (xy 7.9121 -5.08)
				)
				(stroke
					(width 0.2032)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -13.97 5.08 0)
				(length 7.62)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -13.97 2.54 0)
				(length 7.62)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -13.97 0 0)
				(length 7.62)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 13.97 5.08 180)
				(length 7.62)
				(name "PGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 13.97 2.54 180)
				(length 7.62)
				(name "AGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 13.97 0 180)
				(length 7.62)
				(name "SNS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 13.97 -2.54 180)
				(length 7.62)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 13.97 -5.08 180)
				(length 7.62)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "MIC23150-SYMT-TR_1_1"
			(rectangle
				(start -6.35 7.62)
				(end 6.35 -7.62)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
)
