(footprint "IRSensor"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LED, diameter 5.0mm, horizontal offset 1.27mm, z-position of LED center 3.0mm, 2 pins, infrared, black, generated by kicad-footprint-generator")
	(tags "LED IR")
	(property "Reference" "REF**"
		(at 1.27 -1.96 0)
		(layer "F.SilkS")
		(uuid "70d7ec83-4362-4fb9-ab16-a5b0a5594936")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "IRSensor"
		(at 1.27 10.93 0)
		(layer "F.Fab")
		(uuid "faede2b1-a06a-40d0-822d-292f9c20347e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "06c4677f-e4c1-4e34-9384-0539dee5b11a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "fa2ec5b7-21f0-4d81-82c8-ad0f9196c0b1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.29 1.21)
		(end -1.29 7.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "be37698f-7045-4d20-a62b-75eadedfddb8")
	)
	(fp_line
		(start -1.29 1.21)
		(end 3.83 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "69398862-908f-4f21-8e4e-d196fbd04338")
	)
	(fp_line
		(start 0 1.08)
		(end 0 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "97d4d3bf-2a14-4a26-9934-ad4d7f06f836")
	)
	(fp_line
		(start 0 1.21)
		(end 0 1.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "66749608-bfbe-44f6-9107-e6273cb538dc")
	)
	(fp_line
		(start 2.54 1.08)
		(end 2.54 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1df04180-e8f9-4852-991d-8f368c945659")
	)
	(fp_line
		(start 2.54 1.21)
		(end 2.54 1.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "207217ba-7cc4-4c27-b99e-736581b0116f")
	)
	(fp_line
		(start 3.83 1.21)
		(end 3.83 7.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cd5c6212-f41e-4f44-ba74-db4ab4d49435")
	)
	(fp_line
		(start 3.83 1.21)
		(end 4.23 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4a666139-73fe-4f80-93a4-b899e92de4ee")
	)
	(fp_line
		(start 3.83 2.33)
		(end 3.83 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c86225ae-e0d4-4b76-91a1-57aecea565db")
	)
	(fp_line
		(start 4.23 1.21)
		(end 4.23 2.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ac8dfd75-ec5c-4a7a-9a90-c860d337a351")
	)
	(fp_line
		(start 4.23 2.33)
		(end 3.83 2.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "463f0db8-d46e-4923-ae90-6a3b127ea886")
	)
	(fp_arc
		(start 3.83 7.37)
		(mid 1.27 9.93)
		(end -1.29 7.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9c45f4d9-92a2-4091-bdbf-8ecec4e0206a")
	)
	(fp_line
		(start -1.94 -1.21)
		(end -1.94 10.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9340c82f-d67c-4a88-9767-8632c216dd69")
	)
	(fp_line
		(start -1.94 10.18)
		(end 4.49 10.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2b7874e5-61dd-456d-aa02-84c4d581d0e1")
	)
	(fp_line
		(start 4.49 -1.21)
		(end -1.94 -1.21)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b1dbcdd4-7bcd-47b9-b4ff-8c6ab7e7ecba")
	)
	(fp_line
		(start 4.49 10.18)
		(end 4.49 -1.21)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "82325810-ab12-4948-a060-3f26fb981f4c")
	)
	(fp_line
		(start -1.23 1.27)
		(end -1.23 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ba2ca139-8989-4e90-aecc-a61518241303")
	)
	(fp_line
		(start -1.23 1.27)
		(end 3.77 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1b18343a-c2a4-45ba-91ee-762e99976225")
	)
	(fp_line
		(start 0 0)
		(end 0 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ba4dd317-91de-4e3e-a6af-79d28c48e5b9")
	)
	(fp_line
		(start 0 1.27)
		(end 0 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cb5aea23-84e2-4f76-9c0e-1ddeda18bff4")
	)
	(fp_line
		(start 2.54 0)
		(end 2.54 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c8997f9a-ca0a-45d0-aa3b-bccd6fb67d7c")
	)
	(fp_line
		(start 2.54 1.27)
		(end 2.54 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "27bbefb2-4e02-4675-8076-67051760aac3")
	)
	(fp_line
		(start 3.77 1.27)
		(end 3.77 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "98b5e1f9-f1b6-40ec-b6a6-db99c1043896")
	)
	(fp_line
		(start 3.77 1.27)
		(end 4.17 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "594203bc-2749-40ea-aa72-8159174ebea1")
	)
	(fp_line
		(start 3.77 2.27)
		(end 3.77 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "08156ad8-5f24-4c98-879e-c1f2b9eb7713")
	)
	(fp_line
		(start 4.17 1.27)
		(end 4.17 2.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a0a4e4ae-e122-4eda-80b6-0efd66bd6e54")
	)
	(fp_line
		(start 4.17 2.27)
		(end 3.77 2.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f2b2a6ea-af96-4a04-ba47-50b5a27dfbec")
	)
	(fp_arc
		(start 3.77 7.37)
		(mid 1.27 9.87)
		(end -1.23 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f3dd0770-82be-4642-8f3f-d12debd075ab")
	)
	(fp_text user "${REFERENCE}"
		(at 1.27 4.77 0)
		(layer "F.Fab")
		(uuid "985d9a83-eba7-4ee1-8b56-9072d9ba28b2")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e135f3f2-c361-4481-8a7c-ba0ed76b109d")
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e77d9267-661c-479c-ad6c-c0f6b4f667e7")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm_IRBlack.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
