(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "MIC23150-SYMT-TR" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 27.94 10.16 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "MIC23150-SYMT-TR" (id 1) (at 27.94 7.62 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "MLF-8_MT_MCH" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "MIC23150-SYMT-TR" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "MIC23150-SYMT-TR" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "MLF-8_MT_MCH MLF-8_MT_MCH-M MLF-8_MT_MCH-L" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MIC23150-SYMT-TR_0_1"
      (polyline
        (pts
          (xy 7.0993 0)
          (xy 6.0579 0.5207)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.0993 0)
          (xy 6.0579 -0.5207)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.0993 -2.54)
          (xy 6.0579 -2.0193)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.0993 -2.54)
          (xy 6.0579 -3.0607)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.0993 -5.08)
          (xy 6.0579 -4.5593)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.0993 -5.08)
          (xy 6.0579 -5.6007)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.7807 -9.6393)
          (xy 49.8221 -10.16)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.7807 -10.6807)
          (xy 49.8221 -10.16)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.7807 -7.0993)
          (xy 49.8221 -7.62)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.7807 -8.1407)
          (xy 49.8221 -7.62)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.7807 -4.5593)
          (xy 49.8221 -5.08)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.7807 -5.6007)
          (xy 49.8221 -5.08)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 5.08)
          (xy 7.62 -15.24)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 -15.24)
          (xy 48.26 -15.24)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.26 -15.24)
          (xy 48.26 5.08)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 48.26 5.08)
          (xy 7.62 5.08)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin output line (at 55.88 -10.16 180) (length 7.62)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 55.88 -7.62 180) (length 7.62)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 0 0) (length 7.62)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 55.88 -5.08 180) (length 7.62)
        (name "SNS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 55.88 -2.54 180) (length 7.62)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -2.54 0) (length 7.62)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 7.62)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 55.88 0 180) (length 7.62)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)

