(footprint "IRLED"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LED, diameter 5.0mm, horizontal offset 1.27mm, z-position of LED center 3.0mm, 2 pins, clear, generated by kicad-footprint-generator")
	(tags "LED")
	(property "Reference" "REF**"
		(at 1.27 -1.96 0)
		(layer "F.SilkS")
		(uuid "b3475fb4-b9f4-4ce2-a76d-a6fbb12bd5bf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "IRLED"
		(at 1.27 10.93 0)
		(layer "F.Fab")
		(uuid "7e5ce056-ac95-4349-a9f3-95825d818363")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "81b8f6d6-63b6-425d-bc0b-c8a4a98e592a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7fa4fbfc-181d-49a9-867d-3ecedb8ddd86")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.29 1.21)
		(end -1.29 7.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "37984cf7-2a86-4fda-8313-a1aab06a5148")
	)
	(fp_line
		(start -1.29 1.21)
		(end 3.83 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "76274a98-8be9-40ab-9201-de3cde8452b9")
	)
	(fp_line
		(start 0 1.08)
		(end 0 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e5f5af70-065a-4795-9f81-796116f75f44")
	)
	(fp_line
		(start 0 1.21)
		(end 0 1.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "085cebe2-4b33-4ce2-a5cc-4a4f92720f79")
	)
	(fp_line
		(start 2.54 1.08)
		(end 2.54 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "606351fd-0400-481e-a13e-4bbbdc420dda")
	)
	(fp_line
		(start 2.54 1.21)
		(end 2.54 1.08)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "37d7da3d-1460-4a07-ad7e-c70d05918a75")
	)
	(fp_line
		(start 3.83 1.21)
		(end 3.83 7.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "55c0fb0e-ed60-443c-8873-cf71a5fed307")
	)
	(fp_line
		(start 3.83 1.21)
		(end 4.23 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "669e24ce-0179-4eaf-bd46-f7c626a48053")
	)
	(fp_line
		(start 3.83 2.33)
		(end 3.83 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5121081f-6bf7-4c9f-b335-2ca419869d69")
	)
	(fp_line
		(start 4.23 1.21)
		(end 4.23 2.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "769cf625-460e-48cc-9fd7-9d083d378a13")
	)
	(fp_line
		(start 4.23 2.33)
		(end 3.83 2.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a49e1d20-3383-4002-a166-0cd2ff515d05")
	)
	(fp_arc
		(start 3.83 7.37)
		(mid 1.27 9.93)
		(end -1.29 7.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6ab9a364-0315-46aa-ac17-d7eda869b28a")
	)
	(fp_line
		(start -1.94 -1.21)
		(end -1.94 10.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fd8e3c8a-9e04-42b9-8ee4-d42c73bd6fd9")
	)
	(fp_line
		(start -1.94 10.18)
		(end 4.49 10.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c04d57f2-318f-42c0-8995-64da7d4773af")
	)
	(fp_line
		(start 4.49 -1.21)
		(end -1.94 -1.21)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b17239e5-b78d-4488-90f7-5d8b1ed4c371")
	)
	(fp_line
		(start 4.49 10.18)
		(end 4.49 -1.21)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d6efba65-a05e-45b3-a751-660eb198e1f3")
	)
	(fp_line
		(start -1.23 1.27)
		(end -1.23 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "62299cce-3a14-4a15-a3f5-ccd2271f7442")
	)
	(fp_line
		(start -1.23 1.27)
		(end 3.77 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f48fca81-b47c-4698-a8fb-08e5be79f7f5")
	)
	(fp_line
		(start 0 0)
		(end 0 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fd35e3e2-9fc6-46b0-9769-41a08b787791")
	)
	(fp_line
		(start 0 1.27)
		(end 0 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a1033e46-fba3-4851-9547-51b034ca177e")
	)
	(fp_line
		(start 2.54 0)
		(end 2.54 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "26dfebe9-aabd-48ef-ae50-5db26950e382")
	)
	(fp_line
		(start 2.54 1.27)
		(end 2.54 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d8f50907-ff76-48b8-9cce-e67946ac739d")
	)
	(fp_line
		(start 3.77 1.27)
		(end 3.77 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e37dacd8-d865-4618-ace2-6a1e2757d9be")
	)
	(fp_line
		(start 3.77 1.27)
		(end 4.17 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "11b6c58b-bd6f-4aea-913f-12fed58f246c")
	)
	(fp_line
		(start 3.77 2.27)
		(end 3.77 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "539b25f1-f2a0-4366-9aff-d8269cdf30eb")
	)
	(fp_line
		(start 4.17 1.27)
		(end 4.17 2.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "897e2bfb-8f67-4b40-a8d6-9a482dd485b1")
	)
	(fp_line
		(start 4.17 2.27)
		(end 3.77 2.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "080bab5a-28c1-42d4-bd6e-3a08f60b521a")
	)
	(fp_arc
		(start 3.77 7.37)
		(mid 1.27 9.87)
		(end -1.23 7.37)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a55d9ba5-bc25-4c2f-9682-fb90fc73ac70")
	)
	(fp_text user "${REFERENCE}"
		(at 1.27 4.77 0)
		(layer "F.Fab")
		(uuid "b949840d-4a1f-4919-a22e-ff436ea44c0c")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b75e81c7-2ca8-4ee6-82de-b051222f1635")
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b7a0c7e-3f85-47e3-8ef4-4bdfc53b231b")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm_Clear.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
